Next: Frame Filter Management, Previous: Selection, Up: Stack [Contents][Index]

### 8.4 Information About a Frame

There are several other commands to print information about the selected stack frame.

`frame`
`f`

  When used without any argument, this command does not change which frame is selected, but prints a brief description of the currently selected stack frame. It can be abbreviated `f`. With an argument, this command is used to select a stack frame. See Selecting a Frame.

`info frame`
`info f`

  This command prints a verbose description of the selected stack frame, including:

  - the address of the frame
  - the address of the next frame down (called by this frame)
  - the address of the next frame up (caller of this frame)
  - the language in which the source code corresponding to this frame is written
  - the address of the frame’s arguments
  - the address of the frame’s local variables
  - the program counter saved in it (the address of execution in the caller frame)
  - which registers were saved in the frame

  The verbose description is useful when something has gone wrong that has made the stack format fail to fit the usual conventions.

`info frame addr`
`info f addr`

  Print a verbose description of the frame at address addr, without selecting that frame. The selected frame remains unchanged by this command. This requires the same kind of address (more than one for some architectures) that you specify in the `frame` command. See Selecting a Frame.

`info args`

  Print the arguments of the selected frame, each on a separate line.

`info locals`

  Print the local variables of the selected frame, each on a separate line. These are all variables (declared either static or automatic) accessible at the point of execution of the selected frame.

Next: Frame Filter Management, Previous: Selection, Up: Stack [Contents][Index]