Next: SCORE-Pseudo, Up: SCORE-Dependent [Contents][Index]

#### 9.41.1 Options

The following table lists all available SCORE options.

`-G num`

  This option sets the largest size of an object that can be referenced implicitly with the `gp` register. The default value is 8.

`-EB`

  Assemble code for a big-endian cpu

`-EL`

  Assemble code for a little-endian cpu

`-FIXDD`

  Assemble code for fix data dependency

`-NWARN`

  Assemble code for no warning message for fix data dependency

`-SCORE5`

  Assemble code for target is SCORE5

`-SCORE5U`

  Assemble code for target is SCORE5U

`-SCORE7`

  Assemble code for target is SCORE7, this is default setting

`-SCORE3`

  Assemble code for target is SCORE3

`-march=score7`

  Assemble code for target is SCORE7, this is default setting

`-march=score3`

  Assemble code for target is SCORE3

`-USE_R1`

  Assemble code for no warning message when using temp register r1

`-KPIC`

  Generate code for PIC. This option tells the assembler to generate score position-independent macro expansions. It also tells the assembler to mark the output file as PIC.

`-O0`

  Assembler will not perform any optimizations

`-V`

  Sunplus release version