Next: RX Function Attributes, Previous: PowerPC Function Attributes, Up: Function Attributes [Contents][Index]

#### 6.31.24 RL78 Function Attributes

These function attributes are supported by the RL78 back end:

`interrupt`
`brk_interrupt`

  These attributes indicate that the specified function is an interrupt handler. The compiler generates function entry and exit sequences suitable for use in an interrupt handler when this attribute is present.

  Use `brk_interrupt` instead of `interrupt` for handlers intended to be used with the `BRK` opcode (i.e. those that must end with `RETB` instead of `RETI`).

`naked`

  This attribute allows the compiler to construct the requisite function declaration, while allowing the body of the function to be assembly code. The specified function will not have prologue/epilogue sequences generated by the compiler. Only basic `asm` statements can safely be included in naked functions (see Basic Asm). While using extended `asm` or a mixture of basic `asm` and C code may appear to work, they cannot be depended upon to work reliably and are not supported.