Previous: typedef arelent, Up: Relocations [Contents][Index]

#### 2.10.2 The howto manager

When an application wants to create a relocation, but doesn’t know what the target machine might call it, it can find out by using this bit of code.

#### 2.10.2.1 `bfd_reloc_code_type`

Description
The insides of a reloc code. The idea is that, eventually, there will be one enumerator for every type of relocation we ever do. Pass one of these values to `bfd_reloc_type_lookup`, and it’ll return a howto pointer.

This does mean that the application must determine the correct enumerator value; you can’t get a howto pointer from a random set of attributes.

Here are the possible values for `enum bfd_reloc_code_real`:

: BFD_RELOC_64
: BFD_RELOC_32
: BFD_RELOC_26
: BFD_RELOC_24
: BFD_RELOC_16
: BFD_RELOC_14
: BFD_RELOC_8

  Basic absolute relocations of N bits.

: BFD_RELOC_64_PCREL
: BFD_RELOC_32_PCREL
: BFD_RELOC_24_PCREL
: BFD_RELOC_16_PCREL
: BFD_RELOC_12_PCREL
: BFD_RELOC_8_PCREL

  PC-relative relocations. Sometimes these are relative to the address of the relocation itself; sometimes they are relative to the start of the section containing the relocation. It depends on the specific target.

  The 24-bit relocation is used in some Intel 960 configurations.

: BFD_RELOC_32_SECREL

  Section relative relocations. Some targets need this for DWARF2.

: BFD_RELOC_32_GOT_PCREL
: BFD_RELOC_16_GOT_PCREL
: BFD_RELOC_8_GOT_PCREL
: BFD_RELOC_32_GOTOFF
: BFD_RELOC_16_GOTOFF
: BFD_RELOC_LO16_GOTOFF
: BFD_RELOC_HI16_GOTOFF
: BFD_RELOC_HI16_S_GOTOFF
: BFD_RELOC_8_GOTOFF
: BFD_RELOC_64_PLT_PCREL
: BFD_RELOC_32_PLT_PCREL
: BFD_RELOC_24_PLT_PCREL
: BFD_RELOC_16_PLT_PCREL
: BFD_RELOC_8_PLT_PCREL
: BFD_RELOC_64_PLTOFF
: BFD_RELOC_32_PLTOFF
: BFD_RELOC_16_PLTOFF
: BFD_RELOC_LO16_PLTOFF
: BFD_RELOC_HI16_PLTOFF
: BFD_RELOC_HI16_S_PLTOFF
: BFD_RELOC_8_PLTOFF

  For ELF.

: BFD_RELOC_SIZE32
: BFD_RELOC_SIZE64

  Size relocations.

: BFD_RELOC_68K_GLOB_DAT
: BFD_RELOC_68K_JMP_SLOT
: BFD_RELOC_68K_RELATIVE
: BFD_RELOC_68K_TLS_GD32
: BFD_RELOC_68K_TLS_GD16
: BFD_RELOC_68K_TLS_GD8
: BFD_RELOC_68K_TLS_LDM32
: BFD_RELOC_68K_TLS_LDM16
: BFD_RELOC_68K_TLS_LDM8
: BFD_RELOC_68K_TLS_LDO32
: BFD_RELOC_68K_TLS_LDO16
: BFD_RELOC_68K_TLS_LDO8
: BFD_RELOC_68K_TLS_IE32
: BFD_RELOC_68K_TLS_IE16
: BFD_RELOC_68K_TLS_IE8
: BFD_RELOC_68K_TLS_LE32
: BFD_RELOC_68K_TLS_LE16
: BFD_RELOC_68K_TLS_LE8

  Relocations used by 68K ELF.

: BFD_RELOC_32_BASEREL
: BFD_RELOC_16_BASEREL
: BFD_RELOC_LO16_BASEREL
: BFD_RELOC_HI16_BASEREL
: BFD_RELOC_HI16_S_BASEREL
: BFD_RELOC_8_BASEREL
: BFD_RELOC_RVA

  Linkage-table relative.

: BFD_RELOC_8_FFnn

  Absolute 8-bit relocation, but used to form an address like 0xFFnn.

: BFD_RELOC_32_PCREL_S2
: BFD_RELOC_16_PCREL_S2
: BFD_RELOC_23_PCREL_S2

  These PC-relative relocations are stored as word displacements – i.e., byte displacements shifted right two bits. The 30-bit word displacement (<<32_PCREL_S2>> – 32 bits, shifted 2) is used on the SPARC. (SPARC tools generally refer to this as <<WDISP30>>.) The signed 16-bit displacement is used on the MIPS, and the 23-bit displacement is used on the Alpha.

: BFD_RELOC_HI22
: BFD_RELOC_LO10

  High 22 bits and low 10 bits of 32-bit value, placed into lower bits of the target word. These are used on the SPARC.

: BFD_RELOC_GPREL16
: BFD_RELOC_GPREL32

  For systems that allocate a Global Pointer register, these are displacements off that register. These relocation types are handled specially, because the value the register will have is decided relatively late.

: BFD_RELOC_I960_CALLJ

  Reloc types used for i960/b.out.

: BFD_RELOC_NONE
: BFD_RELOC_SPARC_WDISP22
: BFD_RELOC_SPARC22
: BFD_RELOC_SPARC13
: BFD_RELOC_SPARC_GOT10
: BFD_RELOC_SPARC_GOT13
: BFD_RELOC_SPARC_GOT22
: BFD_RELOC_SPARC_PC10
: BFD_RELOC_SPARC_PC22
: BFD_RELOC_SPARC_WPLT30
: BFD_RELOC_SPARC_COPY
: BFD_RELOC_SPARC_GLOB_DAT
: BFD_RELOC_SPARC_JMP_SLOT
: BFD_RELOC_SPARC_RELATIVE
: BFD_RELOC_SPARC_UA16
: BFD_RELOC_SPARC_UA32
: BFD_RELOC_SPARC_UA64
: BFD_RELOC_SPARC_GOTDATA_HIX22
: BFD_RELOC_SPARC_GOTDATA_LOX10
: BFD_RELOC_SPARC_GOTDATA_OP_HIX22
: BFD_RELOC_SPARC_GOTDATA_OP_LOX10
: BFD_RELOC_SPARC_GOTDATA_OP
: BFD_RELOC_SPARC_JMP_IREL
: BFD_RELOC_SPARC_IRELATIVE

  SPARC ELF relocations. There is probably some overlap with other relocation types already defined.

: BFD_RELOC_SPARC_BASE13
: BFD_RELOC_SPARC_BASE22

  I think these are specific to SPARC a.out (e.g., Sun 4).

: BFD_RELOC_SPARC_64
: BFD_RELOC_SPARC_10
: BFD_RELOC_SPARC_11
: BFD_RELOC_SPARC_OLO10
: BFD_RELOC_SPARC_HH22
: BFD_RELOC_SPARC_HM10
: BFD_RELOC_SPARC_LM22
: BFD_RELOC_SPARC_PC_HH22
: BFD_RELOC_SPARC_PC_HM10
: BFD_RELOC_SPARC_PC_LM22
: BFD_RELOC_SPARC_WDISP16
: BFD_RELOC_SPARC_WDISP19
: BFD_RELOC_SPARC_7
: BFD_RELOC_SPARC_6
: BFD_RELOC_SPARC_5
: BFD_RELOC_SPARC_DISP64
: BFD_RELOC_SPARC_PLT32
: BFD_RELOC_SPARC_PLT64
: BFD_RELOC_SPARC_HIX22
: BFD_RELOC_SPARC_LOX10
: BFD_RELOC_SPARC_H44
: BFD_RELOC_SPARC_M44
: BFD_RELOC_SPARC_L44
: BFD_RELOC_SPARC_REGISTER
: BFD_RELOC_SPARC_H34
: BFD_RELOC_SPARC_SIZE32
: BFD_RELOC_SPARC_SIZE64
: BFD_RELOC_SPARC_WDISP10

  SPARC64 relocations

: BFD_RELOC_SPARC_REV32

  SPARC little endian relocation

: BFD_RELOC_SPARC_TLS_GD_HI22
: BFD_RELOC_SPARC_TLS_GD_LO10
: BFD_RELOC_SPARC_TLS_GD_ADD
: BFD_RELOC_SPARC_TLS_GD_CALL
: BFD_RELOC_SPARC_TLS_LDM_HI22
: BFD_RELOC_SPARC_TLS_LDM_LO10
: BFD_RELOC_SPARC_TLS_LDM_ADD
: BFD_RELOC_SPARC_TLS_LDM_CALL
: BFD_RELOC_SPARC_TLS_LDO_HIX22
: BFD_RELOC_SPARC_TLS_LDO_LOX10
: BFD_RELOC_SPARC_TLS_LDO_ADD
: BFD_RELOC_SPARC_TLS_IE_HI22
: BFD_RELOC_SPARC_TLS_IE_LO10
: BFD_RELOC_SPARC_TLS_IE_LD
: BFD_RELOC_SPARC_TLS_IE_LDX
: BFD_RELOC_SPARC_TLS_IE_ADD
: BFD_RELOC_SPARC_TLS_LE_HIX22
: BFD_RELOC_SPARC_TLS_LE_LOX10
: BFD_RELOC_SPARC_TLS_DTPMOD32
: BFD_RELOC_SPARC_TLS_DTPMOD64
: BFD_RELOC_SPARC_TLS_DTPOFF32
: BFD_RELOC_SPARC_TLS_DTPOFF64
: BFD_RELOC_SPARC_TLS_TPOFF32
: BFD_RELOC_SPARC_TLS_TPOFF64

  SPARC TLS relocations

: BFD_RELOC_SPU_IMM7
: BFD_RELOC_SPU_IMM8
: BFD_RELOC_SPU_IMM10
: BFD_RELOC_SPU_IMM10W
: BFD_RELOC_SPU_IMM16
: BFD_RELOC_SPU_IMM16W
: BFD_RELOC_SPU_IMM18
: BFD_RELOC_SPU_PCREL9a
: BFD_RELOC_SPU_PCREL9b
: BFD_RELOC_SPU_PCREL16
: BFD_RELOC_SPU_LO16
: BFD_RELOC_SPU_HI16
: BFD_RELOC_SPU_PPU32
: BFD_RELOC_SPU_PPU64
: BFD_RELOC_SPU_ADD_PIC

  SPU Relocations.

: BFD_RELOC_ALPHA_GPDISP_HI16

  Alpha ECOFF and ELF relocations. Some of these treat the symbol or "addend" in some special way. For GPDISP_HI16 ("gpdisp") relocations, the symbol is ignored when writing; when reading, it will be the absolute section symbol. The addend is the displacement in bytes of the "lda" instruction from the "ldah" instruction (which is at the address of this reloc).

: BFD_RELOC_ALPHA_GPDISP_LO16

  For GPDISP_LO16 ("ignore") relocations, the symbol is handled as with GPDISP_HI16 relocs. The addend is ignored when writing the relocations out, and is filled in with the file’s GP value on reading, for convenience.

: BFD_RELOC_ALPHA_GPDISP

  The ELF GPDISP relocation is exactly the same as the GPDISP_HI16 relocation except that there is no accompanying GPDISP_LO16 relocation.

: BFD_RELOC_ALPHA_LITERAL
: BFD_RELOC_ALPHA_ELF_LITERAL
: BFD_RELOC_ALPHA_LITUSE

  The Alpha LITERAL/LITUSE relocs are produced by a symbol reference; the assembler turns it into a LDQ instruction to load the address of the symbol, and then fills in a register in the real instruction.

  The LITERAL reloc, at the LDQ instruction, refers to the .lita section symbol. The addend is ignored when writing, but is filled in with the file’s GP value on reading, for convenience, as with the GPDISP_LO16 reloc.

  The ELF_LITERAL reloc is somewhere between 16_GOTOFF and GPDISP_LO16. It should refer to the symbol to be referenced, as with 16_GOTOFF, but it generates output not based on the position within the .got section, but relative to the GP value chosen for the file during the final link stage.

  The LITUSE reloc, on the instruction using the loaded address, gives information to the linker that it might be able to use to optimize away some literal section references. The symbol is ignored (read as the absolute section symbol), and the "addend" indicates the type of instruction using the register: 1 - "memory" fmt insn 2 - byte-manipulation (byte offset reg) 3 - jsr (target of branch)

: BFD_RELOC_ALPHA_HINT

  The HINT relocation indicates a value that should be filled into the "hint" field of a jmp/jsr/ret instruction, for possible branch- prediction logic which may be provided on some processors.

: BFD_RELOC_ALPHA_LINKAGE

  The LINKAGE relocation outputs a linkage pair in the object file, which is filled by the linker.

: BFD_RELOC_ALPHA_CODEADDR

  The CODEADDR relocation outputs a STO_CA in the object file, which is filled by the linker.

: BFD_RELOC_ALPHA_GPREL_HI16
: BFD_RELOC_ALPHA_GPREL_LO16

  The GPREL_HI/LO relocations together form a 32-bit offset from the GP register.

: BFD_RELOC_ALPHA_BRSGP

  Like BFD_RELOC_23_PCREL_S2, except that the source and target must share a common GP, and the target address is adjusted for STO_ALPHA_STD_GPLOAD.

: BFD_RELOC_ALPHA_NOP

  The NOP relocation outputs a NOP if the longword displacement between two procedure entry points is < 2^21.

: BFD_RELOC_ALPHA_BSR

  The BSR relocation outputs a BSR if the longword displacement between two procedure entry points is < 2^21.

: BFD_RELOC_ALPHA_LDA

  The LDA relocation outputs a LDA if the longword displacement between two procedure entry points is < 2^16.

: BFD_RELOC_ALPHA_BOH

  The BOH relocation outputs a BSR if the longword displacement between two procedure entry points is < 2^21, or else a hint.

: BFD_RELOC_ALPHA_TLSGD
: BFD_RELOC_ALPHA_TLSLDM
: BFD_RELOC_ALPHA_DTPMOD64
: BFD_RELOC_ALPHA_GOTDTPREL16
: BFD_RELOC_ALPHA_DTPREL64
: BFD_RELOC_ALPHA_DTPREL_HI16
: BFD_RELOC_ALPHA_DTPREL_LO16
: BFD_RELOC_ALPHA_DTPREL16
: BFD_RELOC_ALPHA_GOTTPREL16
: BFD_RELOC_ALPHA_TPREL64
: BFD_RELOC_ALPHA_TPREL_HI16
: BFD_RELOC_ALPHA_TPREL_LO16
: BFD_RELOC_ALPHA_TPREL16

  Alpha thread-local storage relocations.

: BFD_RELOC_MIPS_JMP
: BFD_RELOC_MICROMIPS_JMP

  The MIPS jump instruction.

: BFD_RELOC_MIPS16_JMP

  The MIPS16 jump instruction.

: BFD_RELOC_MIPS16_GPREL

  MIPS16 GP relative reloc.

: BFD_RELOC_HI16

  High 16 bits of 32-bit value; simple reloc.

: BFD_RELOC_HI16_S

  High 16 bits of 32-bit value but the low 16 bits will be sign extended and added to form the final result. If the low 16 bits form a negative number, we need to add one to the high value to compensate for the borrow when the low bits are added.

: BFD_RELOC_LO16

  Low 16 bits.

: BFD_RELOC_HI16_PCREL

  High 16 bits of 32-bit pc-relative value

: BFD_RELOC_HI16_S_PCREL

  High 16 bits of 32-bit pc-relative value, adjusted

: BFD_RELOC_LO16_PCREL

  Low 16 bits of pc-relative value

: BFD_RELOC_MIPS16_GOT16
: BFD_RELOC_MIPS16_CALL16

  Equivalent of BFD_RELOC_MIPS_*, but with the MIPS16 layout of 16-bit immediate fields

: BFD_RELOC_MIPS16_HI16

  MIPS16 high 16 bits of 32-bit value.

: BFD_RELOC_MIPS16_HI16_S

  MIPS16 high 16 bits of 32-bit value but the low 16 bits will be sign extended and added to form the final result. If the low 16 bits form a negative number, we need to add one to the high value to compensate for the borrow when the low bits are added.

: BFD_RELOC_MIPS16_LO16

  MIPS16 low 16 bits.

: BFD_RELOC_MIPS16_TLS_GD
: BFD_RELOC_MIPS16_TLS_LDM
: BFD_RELOC_MIPS16_TLS_DTPREL_HI16
: BFD_RELOC_MIPS16_TLS_DTPREL_LO16
: BFD_RELOC_MIPS16_TLS_GOTTPREL
: BFD_RELOC_MIPS16_TLS_TPREL_HI16
: BFD_RELOC_MIPS16_TLS_TPREL_LO16

  MIPS16 TLS relocations

: BFD_RELOC_MIPS_LITERAL
: BFD_RELOC_MICROMIPS_LITERAL

  Relocation against a MIPS literal section.

: BFD_RELOC_MICROMIPS_7_PCREL_S1
: BFD_RELOC_MICROMIPS_10_PCREL_S1
: BFD_RELOC_MICROMIPS_16_PCREL_S1

  microMIPS PC-relative relocations.

: BFD_RELOC_MIPS16_16_PCREL_S1

  MIPS16 PC-relative relocation.

: BFD_RELOC_MIPS_21_PCREL_S2
: BFD_RELOC_MIPS_26_PCREL_S2
: BFD_RELOC_MIPS_18_PCREL_S3
: BFD_RELOC_MIPS_19_PCREL_S2

  MIPS PC-relative relocations.

: BFD_RELOC_MICROMIPS_GPREL16
: BFD_RELOC_MICROMIPS_HI16
: BFD_RELOC_MICROMIPS_HI16_S
: BFD_RELOC_MICROMIPS_LO16

  microMIPS versions of generic BFD relocs.

: BFD_RELOC_MIPS_GOT16
: BFD_RELOC_MICROMIPS_GOT16
: BFD_RELOC_MIPS_CALL16
: BFD_RELOC_MICROMIPS_CALL16
: BFD_RELOC_MIPS_GOT_HI16
: BFD_RELOC_MICROMIPS_GOT_HI16
: BFD_RELOC_MIPS_GOT_LO16
: BFD_RELOC_MICROMIPS_GOT_LO16
: BFD_RELOC_MIPS_CALL_HI16
: BFD_RELOC_MICROMIPS_CALL_HI16
: BFD_RELOC_MIPS_CALL_LO16
: BFD_RELOC_MICROMIPS_CALL_LO16
: BFD_RELOC_MIPS_SUB
: BFD_RELOC_MICROMIPS_SUB
: BFD_RELOC_MIPS_GOT_PAGE
: BFD_RELOC_MICROMIPS_GOT_PAGE
: BFD_RELOC_MIPS_GOT_OFST
: BFD_RELOC_MICROMIPS_GOT_OFST
: BFD_RELOC_MIPS_GOT_DISP
: BFD_RELOC_MICROMIPS_GOT_DISP
: BFD_RELOC_MIPS_SHIFT5
: BFD_RELOC_MIPS_SHIFT6
: BFD_RELOC_MIPS_INSERT_A
: BFD_RELOC_MIPS_INSERT_B
: BFD_RELOC_MIPS_DELETE
: BFD_RELOC_MIPS_HIGHEST
: BFD_RELOC_MICROMIPS_HIGHEST
: BFD_RELOC_MIPS_HIGHER
: BFD_RELOC_MICROMIPS_HIGHER
: BFD_RELOC_MIPS_SCN_DISP
: BFD_RELOC_MICROMIPS_SCN_DISP
: BFD_RELOC_MIPS_REL16
: BFD_RELOC_MIPS_RELGOT
: BFD_RELOC_MIPS_JALR
: BFD_RELOC_MICROMIPS_JALR
: BFD_RELOC_MIPS_TLS_DTPMOD32
: BFD_RELOC_MIPS_TLS_DTPREL32
: BFD_RELOC_MIPS_TLS_DTPMOD64
: BFD_RELOC_MIPS_TLS_DTPREL64
: BFD_RELOC_MIPS_TLS_GD
: BFD_RELOC_MICROMIPS_TLS_GD
: BFD_RELOC_MIPS_TLS_LDM
: BFD_RELOC_MICROMIPS_TLS_LDM
: BFD_RELOC_MIPS_TLS_DTPREL_HI16
: BFD_RELOC_MICROMIPS_TLS_DTPREL_HI16
: BFD_RELOC_MIPS_TLS_DTPREL_LO16
: BFD_RELOC_MICROMIPS_TLS_DTPREL_LO16
: BFD_RELOC_MIPS_TLS_GOTTPREL
: BFD_RELOC_MICROMIPS_TLS_GOTTPREL
: BFD_RELOC_MIPS_TLS_TPREL32
: BFD_RELOC_MIPS_TLS_TPREL64
: BFD_RELOC_MIPS_TLS_TPREL_HI16
: BFD_RELOC_MICROMIPS_TLS_TPREL_HI16
: BFD_RELOC_MIPS_TLS_TPREL_LO16
: BFD_RELOC_MICROMIPS_TLS_TPREL_LO16
: BFD_RELOC_MIPS_EH

  MIPS ELF relocations.

: BFD_RELOC_MIPS_COPY
: BFD_RELOC_MIPS_JUMP_SLOT

  MIPS ELF relocations (VxWorks and PLT extensions).

: BFD_RELOC_MOXIE_10_PCREL

  Moxie ELF relocations.

: BFD_RELOC_FT32_10
: BFD_RELOC_FT32_20
: BFD_RELOC_FT32_17
: BFD_RELOC_FT32_18
: BFD_RELOC_FT32_RELAX
: BFD_RELOC_FT32_SC0
: BFD_RELOC_FT32_SC1
: BFD_RELOC_FT32_15
: BFD_RELOC_FT32_DIFF32

  FT32 ELF relocations.

: BFD_RELOC_FRV_LABEL16
: BFD_RELOC_FRV_LABEL24
: BFD_RELOC_FRV_LO16
: BFD_RELOC_FRV_HI16
: BFD_RELOC_FRV_GPREL12
: BFD_RELOC_FRV_GPRELU12
: BFD_RELOC_FRV_GPREL32
: BFD_RELOC_FRV_GPRELHI
: BFD_RELOC_FRV_GPRELLO
: BFD_RELOC_FRV_GOT12
: BFD_RELOC_FRV_GOTHI
: BFD_RELOC_FRV_GOTLO
: BFD_RELOC_FRV_FUNCDESC
: BFD_RELOC_FRV_FUNCDESC_GOT12
: BFD_RELOC_FRV_FUNCDESC_GOTHI
: BFD_RELOC_FRV_FUNCDESC_GOTLO
: BFD_RELOC_FRV_FUNCDESC_VALUE
: BFD_RELOC_FRV_FUNCDESC_GOTOFF12
: BFD_RELOC_FRV_FUNCDESC_GOTOFFHI
: BFD_RELOC_FRV_FUNCDESC_GOTOFFLO
: BFD_RELOC_FRV_GOTOFF12
: BFD_RELOC_FRV_GOTOFFHI
: BFD_RELOC_FRV_GOTOFFLO
: BFD_RELOC_FRV_GETTLSOFF
: BFD_RELOC_FRV_TLSDESC_VALUE
: BFD_RELOC_FRV_GOTTLSDESC12
: BFD_RELOC_FRV_GOTTLSDESCHI
: BFD_RELOC_FRV_GOTTLSDESCLO
: BFD_RELOC_FRV_TLSMOFF12
: BFD_RELOC_FRV_TLSMOFFHI
: BFD_RELOC_FRV_TLSMOFFLO
: BFD_RELOC_FRV_GOTTLSOFF12
: BFD_RELOC_FRV_GOTTLSOFFHI
: BFD_RELOC_FRV_GOTTLSOFFLO
: BFD_RELOC_FRV_TLSOFF
: BFD_RELOC_FRV_TLSDESC_RELAX
: BFD_RELOC_FRV_GETTLSOFF_RELAX
: BFD_RELOC_FRV_TLSOFF_RELAX
: BFD_RELOC_FRV_TLSMOFF

  Fujitsu Frv Relocations.

: BFD_RELOC_MN10300_GOTOFF24

  This is a 24bit GOT-relative reloc for the mn10300.

: BFD_RELOC_MN10300_GOT32

  This is a 32bit GOT-relative reloc for the mn10300, offset by two bytes in the instruction.

: BFD_RELOC_MN10300_GOT24

  This is a 24bit GOT-relative reloc for the mn10300, offset by two bytes in the instruction.

: BFD_RELOC_MN10300_GOT16

  This is a 16bit GOT-relative reloc for the mn10300, offset by two bytes in the instruction.

: BFD_RELOC_MN10300_COPY

  Copy symbol at runtime.

: BFD_RELOC_MN10300_GLOB_DAT

  Create GOT entry.

: BFD_RELOC_MN10300_JMP_SLOT

  Create PLT entry.

: BFD_RELOC_MN10300_RELATIVE

  Adjust by program base.

: BFD_RELOC_MN10300_SYM_DIFF

  Together with another reloc targeted at the same location, allows for a value that is the difference of two symbols in the same section.

: BFD_RELOC_MN10300_ALIGN

  The addend of this reloc is an alignment power that must be honoured at the offset’s location, regardless of linker relaxation.

: BFD_RELOC_MN10300_TLS_GD
: BFD_RELOC_MN10300_TLS_LD
: BFD_RELOC_MN10300_TLS_LDO
: BFD_RELOC_MN10300_TLS_GOTIE
: BFD_RELOC_MN10300_TLS_IE
: BFD_RELOC_MN10300_TLS_LE
: BFD_RELOC_MN10300_TLS_DTPMOD
: BFD_RELOC_MN10300_TLS_DTPOFF
: BFD_RELOC_MN10300_TLS_TPOFF

  Various TLS-related relocations.

: BFD_RELOC_MN10300_32_PCREL

  This is a 32bit pcrel reloc for the mn10300, offset by two bytes in the instruction.

: BFD_RELOC_MN10300_16_PCREL

  This is a 16bit pcrel reloc for the mn10300, offset by two bytes in the instruction.

: BFD_RELOC_386_GOT32
: BFD_RELOC_386_PLT32
: BFD_RELOC_386_COPY
: BFD_RELOC_386_GLOB_DAT
: BFD_RELOC_386_JUMP_SLOT
: BFD_RELOC_386_RELATIVE
: BFD_RELOC_386_GOTOFF
: BFD_RELOC_386_GOTPC
: BFD_RELOC_386_TLS_TPOFF
: BFD_RELOC_386_TLS_IE
: BFD_RELOC_386_TLS_GOTIE
: BFD_RELOC_386_TLS_LE
: BFD_RELOC_386_TLS_GD
: BFD_RELOC_386_TLS_LDM
: BFD_RELOC_386_TLS_LDO_32
: BFD_RELOC_386_TLS_IE_32
: BFD_RELOC_386_TLS_LE_32
: BFD_RELOC_386_TLS_DTPMOD32
: BFD_RELOC_386_TLS_DTPOFF32
: BFD_RELOC_386_TLS_TPOFF32
: BFD_RELOC_386_TLS_GOTDESC
: BFD_RELOC_386_TLS_DESC_CALL
: BFD_RELOC_386_TLS_DESC
: BFD_RELOC_386_IRELATIVE
: BFD_RELOC_386_GOT32X

  i386/elf relocations

: BFD_RELOC_X86_64_GOT32
: BFD_RELOC_X86_64_PLT32
: BFD_RELOC_X86_64_COPY
: BFD_RELOC_X86_64_GLOB_DAT
: BFD_RELOC_X86_64_JUMP_SLOT
: BFD_RELOC_X86_64_RELATIVE
: BFD_RELOC_X86_64_GOTPCREL
: BFD_RELOC_X86_64_32S
: BFD_RELOC_X86_64_DTPMOD64
: BFD_RELOC_X86_64_DTPOFF64
: BFD_RELOC_X86_64_TPOFF64
: BFD_RELOC_X86_64_TLSGD
: BFD_RELOC_X86_64_TLSLD
: BFD_RELOC_X86_64_DTPOFF32
: BFD_RELOC_X86_64_GOTTPOFF
: BFD_RELOC_X86_64_TPOFF32
: BFD_RELOC_X86_64_GOTOFF64
: BFD_RELOC_X86_64_GOTPC32
: BFD_RELOC_X86_64_GOT64
: BFD_RELOC_X86_64_GOTPCREL64
: BFD_RELOC_X86_64_GOTPC64
: BFD_RELOC_X86_64_GOTPLT64
: BFD_RELOC_X86_64_PLTOFF64
: BFD_RELOC_X86_64_GOTPC32_TLSDESC
: BFD_RELOC_X86_64_TLSDESC_CALL
: BFD_RELOC_X86_64_TLSDESC
: BFD_RELOC_X86_64_IRELATIVE
: BFD_RELOC_X86_64_PC32_BND
: BFD_RELOC_X86_64_PLT32_BND
: BFD_RELOC_X86_64_GOTPCRELX
: BFD_RELOC_X86_64_REX_GOTPCRELX

  x86-64/elf relocations

: BFD_RELOC_NS32K_IMM_8
: BFD_RELOC_NS32K_IMM_16
: BFD_RELOC_NS32K_IMM_32
: BFD_RELOC_NS32K_IMM_8_PCREL
: BFD_RELOC_NS32K_IMM_16_PCREL
: BFD_RELOC_NS32K_IMM_32_PCREL
: BFD_RELOC_NS32K_DISP_8
: BFD_RELOC_NS32K_DISP_16
: BFD_RELOC_NS32K_DISP_32
: BFD_RELOC_NS32K_DISP_8_PCREL
: BFD_RELOC_NS32K_DISP_16_PCREL
: BFD_RELOC_NS32K_DISP_32_PCREL

  ns32k relocations

: BFD_RELOC_PDP11_DISP_8_PCREL
: BFD_RELOC_PDP11_DISP_6_PCREL

  PDP11 relocations

: BFD_RELOC_PJ_CODE_HI16
: BFD_RELOC_PJ_CODE_LO16
: BFD_RELOC_PJ_CODE_DIR16
: BFD_RELOC_PJ_CODE_DIR32
: BFD_RELOC_PJ_CODE_REL16
: BFD_RELOC_PJ_CODE_REL32

  Picojava relocs. Not all of these appear in object files.

: BFD_RELOC_PPC_B26
: BFD_RELOC_PPC_BA26
: BFD_RELOC_PPC_TOC16
: BFD_RELOC_PPC_B16
: BFD_RELOC_PPC_B16_BRTAKEN
: BFD_RELOC_PPC_B16_BRNTAKEN
: BFD_RELOC_PPC_BA16
: BFD_RELOC_PPC_BA16_BRTAKEN
: BFD_RELOC_PPC_BA16_BRNTAKEN
: BFD_RELOC_PPC_COPY
: BFD_RELOC_PPC_GLOB_DAT
: BFD_RELOC_PPC_JMP_SLOT
: BFD_RELOC_PPC_RELATIVE
: BFD_RELOC_PPC_LOCAL24PC
: BFD_RELOC_PPC_EMB_NADDR32
: BFD_RELOC_PPC_EMB_NADDR16
: BFD_RELOC_PPC_EMB_NADDR16_LO
: BFD_RELOC_PPC_EMB_NADDR16_HI
: BFD_RELOC_PPC_EMB_NADDR16_HA
: BFD_RELOC_PPC_EMB_SDAI16
: BFD_RELOC_PPC_EMB_SDA2I16
: BFD_RELOC_PPC_EMB_SDA2REL
: BFD_RELOC_PPC_EMB_SDA21
: BFD_RELOC_PPC_EMB_MRKREF
: BFD_RELOC_PPC_EMB_RELSEC16
: BFD_RELOC_PPC_EMB_RELST_LO
: BFD_RELOC_PPC_EMB_RELST_HI
: BFD_RELOC_PPC_EMB_RELST_HA
: BFD_RELOC_PPC_EMB_BIT_FLD
: BFD_RELOC_PPC_EMB_RELSDA
: BFD_RELOC_PPC_VLE_REL8
: BFD_RELOC_PPC_VLE_REL15
: BFD_RELOC_PPC_VLE_REL24
: BFD_RELOC_PPC_VLE_LO16A
: BFD_RELOC_PPC_VLE_LO16D
: BFD_RELOC_PPC_VLE_HI16A
: BFD_RELOC_PPC_VLE_HI16D
: BFD_RELOC_PPC_VLE_HA16A
: BFD_RELOC_PPC_VLE_HA16D
: BFD_RELOC_PPC_VLE_SDA21
: BFD_RELOC_PPC_VLE_SDA21_LO
: BFD_RELOC_PPC_VLE_SDAREL_LO16A
: BFD_RELOC_PPC_VLE_SDAREL_LO16D
: BFD_RELOC_PPC_VLE_SDAREL_HI16A
: BFD_RELOC_PPC_VLE_SDAREL_HI16D
: BFD_RELOC_PPC_VLE_SDAREL_HA16A
: BFD_RELOC_PPC_VLE_SDAREL_HA16D
: BFD_RELOC_PPC_16DX_HA
: BFD_RELOC_PPC_REL16DX_HA
: BFD_RELOC_PPC64_HIGHER
: BFD_RELOC_PPC64_HIGHER_S
: BFD_RELOC_PPC64_HIGHEST
: BFD_RELOC_PPC64_HIGHEST_S
: BFD_RELOC_PPC64_TOC16_LO
: BFD_RELOC_PPC64_TOC16_HI
: BFD_RELOC_PPC64_TOC16_HA
: BFD_RELOC_PPC64_TOC
: BFD_RELOC_PPC64_PLTGOT16
: BFD_RELOC_PPC64_PLTGOT16_LO
: BFD_RELOC_PPC64_PLTGOT16_HI
: BFD_RELOC_PPC64_PLTGOT16_HA
: BFD_RELOC_PPC64_ADDR16_DS
: BFD_RELOC_PPC64_ADDR16_LO_DS
: BFD_RELOC_PPC64_GOT16_DS
: BFD_RELOC_PPC64_GOT16_LO_DS
: BFD_RELOC_PPC64_PLT16_LO_DS
: BFD_RELOC_PPC64_SECTOFF_DS
: BFD_RELOC_PPC64_SECTOFF_LO_DS
: BFD_RELOC_PPC64_TOC16_DS
: BFD_RELOC_PPC64_TOC16_LO_DS
: BFD_RELOC_PPC64_PLTGOT16_DS
: BFD_RELOC_PPC64_PLTGOT16_LO_DS
: BFD_RELOC_PPC64_ADDR16_HIGH
: BFD_RELOC_PPC64_ADDR16_HIGHA
: BFD_RELOC_PPC64_ADDR64_LOCAL
: BFD_RELOC_PPC64_ENTRY

  Power(rs6000) and PowerPC relocations.

: BFD_RELOC_PPC_TLS
: BFD_RELOC_PPC_TLSGD
: BFD_RELOC_PPC_TLSLD
: BFD_RELOC_PPC_DTPMOD
: BFD_RELOC_PPC_TPREL16
: BFD_RELOC_PPC_TPREL16_LO
: BFD_RELOC_PPC_TPREL16_HI
: BFD_RELOC_PPC_TPREL16_HA
: BFD_RELOC_PPC_TPREL
: BFD_RELOC_PPC_DTPREL16
: BFD_RELOC_PPC_DTPREL16_LO
: BFD_RELOC_PPC_DTPREL16_HI
: BFD_RELOC_PPC_DTPREL16_HA
: BFD_RELOC_PPC_DTPREL
: BFD_RELOC_PPC_GOT_TLSGD16
: BFD_RELOC_PPC_GOT_TLSGD16_LO
: BFD_RELOC_PPC_GOT_TLSGD16_HI
: BFD_RELOC_PPC_GOT_TLSGD16_HA
: BFD_RELOC_PPC_GOT_TLSLD16
: BFD_RELOC_PPC_GOT_TLSLD16_LO
: BFD_RELOC_PPC_GOT_TLSLD16_HI
: BFD_RELOC_PPC_GOT_TLSLD16_HA
: BFD_RELOC_PPC_GOT_TPREL16
: BFD_RELOC_PPC_GOT_TPREL16_LO
: BFD_RELOC_PPC_GOT_TPREL16_HI
: BFD_RELOC_PPC_GOT_TPREL16_HA
: BFD_RELOC_PPC_GOT_DTPREL16
: BFD_RELOC_PPC_GOT_DTPREL16_LO
: BFD_RELOC_PPC_GOT_DTPREL16_HI
: BFD_RELOC_PPC_GOT_DTPREL16_HA
: BFD_RELOC_PPC64_TPREL16_DS
: BFD_RELOC_PPC64_TPREL16_LO_DS
: BFD_RELOC_PPC64_TPREL16_HIGHER
: BFD_RELOC_PPC64_TPREL16_HIGHERA
: BFD_RELOC_PPC64_TPREL16_HIGHEST
: BFD_RELOC_PPC64_TPREL16_HIGHESTA
: BFD_RELOC_PPC64_DTPREL16_DS
: BFD_RELOC_PPC64_DTPREL16_LO_DS
: BFD_RELOC_PPC64_DTPREL16_HIGHER
: BFD_RELOC_PPC64_DTPREL16_HIGHERA
: BFD_RELOC_PPC64_DTPREL16_HIGHEST
: BFD_RELOC_PPC64_DTPREL16_HIGHESTA
: BFD_RELOC_PPC64_TPREL16_HIGH
: BFD_RELOC_PPC64_TPREL16_HIGHA
: BFD_RELOC_PPC64_DTPREL16_HIGH
: BFD_RELOC_PPC64_DTPREL16_HIGHA

  PowerPC and PowerPC64 thread-local storage relocations.

: BFD_RELOC_I370_D12

  IBM 370/390 relocations

: BFD_RELOC_CTOR

  The type of reloc used to build a constructor table - at the moment probably a 32 bit wide absolute relocation, but the target can choose. It generally does map to one of the other relocation types.

: BFD_RELOC_ARM_PCREL_BRANCH

  ARM 26 bit pc-relative branch. The lowest two bits must be zero and are not stored in the instruction.

: BFD_RELOC_ARM_PCREL_BLX

  ARM 26 bit pc-relative branch. The lowest bit must be zero and is not stored in the instruction. The 2nd lowest bit comes from a 1 bit field in the instruction.

: BFD_RELOC_THUMB_PCREL_BLX

  Thumb 22 bit pc-relative branch. The lowest bit must be zero and is not stored in the instruction. The 2nd lowest bit comes from a 1 bit field in the instruction.

: BFD_RELOC_ARM_PCREL_CALL

  ARM 26-bit pc-relative branch for an unconditional BL or BLX instruction.

: BFD_RELOC_ARM_PCREL_JUMP

  ARM 26-bit pc-relative branch for B or conditional BL instruction.

: BFD_RELOC_THUMB_PCREL_BRANCH7
: BFD_RELOC_THUMB_PCREL_BRANCH9
: BFD_RELOC_THUMB_PCREL_BRANCH12
: BFD_RELOC_THUMB_PCREL_BRANCH20
: BFD_RELOC_THUMB_PCREL_BRANCH23
: BFD_RELOC_THUMB_PCREL_BRANCH25

  Thumb 7-, 9-, 12-, 20-, 23-, and 25-bit pc-relative branches. The lowest bit must be zero and is not stored in the instruction. Note that the corresponding ELF R_ARM_THM_JUMPnn constant has an "nn" one smaller in all cases. Note further that BRANCH23 corresponds to R_ARM_THM_CALL.

: BFD_RELOC_ARM_OFFSET_IMM

  12-bit immediate offset, used in ARM-format ldr and str instructions.

: BFD_RELOC_ARM_THUMB_OFFSET

  5-bit immediate offset, used in Thumb-format ldr and str instructions.

: BFD_RELOC_ARM_TARGET1

  Pc-relative or absolute relocation depending on target. Used for entries in .init_array sections.

: BFD_RELOC_ARM_ROSEGREL32

  Read-only segment base relative address.

: BFD_RELOC_ARM_SBREL32

  Data segment base relative address.

: BFD_RELOC_ARM_TARGET2

  This reloc is used for references to RTTI data from exception handling tables. The actual definition depends on the target. It may be a pc-relative or some form of GOT-indirect relocation.

: BFD_RELOC_ARM_PREL31

  31-bit PC relative address.

: BFD_RELOC_ARM_MOVW
: BFD_RELOC_ARM_MOVT
: BFD_RELOC_ARM_MOVW_PCREL
: BFD_RELOC_ARM_MOVT_PCREL
: BFD_RELOC_ARM_THUMB_MOVW
: BFD_RELOC_ARM_THUMB_MOVT
: BFD_RELOC_ARM_THUMB_MOVW_PCREL
: BFD_RELOC_ARM_THUMB_MOVT_PCREL

  Low and High halfword relocations for MOVW and MOVT instructions.

: BFD_RELOC_ARM_JUMP_SLOT
: BFD_RELOC_ARM_GLOB_DAT
: BFD_RELOC_ARM_GOT32
: BFD_RELOC_ARM_PLT32
: BFD_RELOC_ARM_RELATIVE
: BFD_RELOC_ARM_GOTOFF
: BFD_RELOC_ARM_GOTPC
: BFD_RELOC_ARM_GOT_PREL

  Relocations for setting up GOTs and PLTs for shared libraries.

: BFD_RELOC_ARM_TLS_GD32
: BFD_RELOC_ARM_TLS_LDO32
: BFD_RELOC_ARM_TLS_LDM32
: BFD_RELOC_ARM_TLS_DTPOFF32
: BFD_RELOC_ARM_TLS_DTPMOD32
: BFD_RELOC_ARM_TLS_TPOFF32
: BFD_RELOC_ARM_TLS_IE32
: BFD_RELOC_ARM_TLS_LE32
: BFD_RELOC_ARM_TLS_GOTDESC
: BFD_RELOC_ARM_TLS_CALL
: BFD_RELOC_ARM_THM_TLS_CALL
: BFD_RELOC_ARM_TLS_DESCSEQ
: BFD_RELOC_ARM_THM_TLS_DESCSEQ
: BFD_RELOC_ARM_TLS_DESC

  ARM thread-local storage relocations.

: BFD_RELOC_ARM_ALU_PC_G0_NC
: BFD_RELOC_ARM_ALU_PC_G0
: BFD_RELOC_ARM_ALU_PC_G1_NC
: BFD_RELOC_ARM_ALU_PC_G1
: BFD_RELOC_ARM_ALU_PC_G2
: BFD_RELOC_ARM_LDR_PC_G0
: BFD_RELOC_ARM_LDR_PC_G1
: BFD_RELOC_ARM_LDR_PC_G2
: BFD_RELOC_ARM_LDRS_PC_G0
: BFD_RELOC_ARM_LDRS_PC_G1
: BFD_RELOC_ARM_LDRS_PC_G2
: BFD_RELOC_ARM_LDC_PC_G0
: BFD_RELOC_ARM_LDC_PC_G1
: BFD_RELOC_ARM_LDC_PC_G2
: BFD_RELOC_ARM_ALU_SB_G0_NC
: BFD_RELOC_ARM_ALU_SB_G0
: BFD_RELOC_ARM_ALU_SB_G1_NC
: BFD_RELOC_ARM_ALU_SB_G1
: BFD_RELOC_ARM_ALU_SB_G2
: BFD_RELOC_ARM_LDR_SB_G0
: BFD_RELOC_ARM_LDR_SB_G1
: BFD_RELOC_ARM_LDR_SB_G2
: BFD_RELOC_ARM_LDRS_SB_G0
: BFD_RELOC_ARM_LDRS_SB_G1
: BFD_RELOC_ARM_LDRS_SB_G2
: BFD_RELOC_ARM_LDC_SB_G0
: BFD_RELOC_ARM_LDC_SB_G1
: BFD_RELOC_ARM_LDC_SB_G2

  ARM group relocations.

: BFD_RELOC_ARM_V4BX

  Annotation of BX instructions.

: BFD_RELOC_ARM_IRELATIVE

  ARM support for STT_GNU_IFUNC.

: BFD_RELOC_ARM_THUMB_ALU_ABS_G0_NC
: BFD_RELOC_ARM_THUMB_ALU_ABS_G1_NC
: BFD_RELOC_ARM_THUMB_ALU_ABS_G2_NC
: BFD_RELOC_ARM_THUMB_ALU_ABS_G3_NC

  Thumb1 relocations to support execute-only code.

: BFD_RELOC_ARM_IMMEDIATE
: BFD_RELOC_ARM_ADRL_IMMEDIATE
: BFD_RELOC_ARM_T32_IMMEDIATE
: BFD_RELOC_ARM_T32_ADD_IMM
: BFD_RELOC_ARM_T32_IMM12
: BFD_RELOC_ARM_T32_ADD_PC12
: BFD_RELOC_ARM_SHIFT_IMM
: BFD_RELOC_ARM_SMC
: BFD_RELOC_ARM_HVC
: BFD_RELOC_ARM_SWI
: BFD_RELOC_ARM_MULTI
: BFD_RELOC_ARM_CP_OFF_IMM
: BFD_RELOC_ARM_CP_OFF_IMM_S2
: BFD_RELOC_ARM_T32_CP_OFF_IMM
: BFD_RELOC_ARM_T32_CP_OFF_IMM_S2
: BFD_RELOC_ARM_ADR_IMM
: BFD_RELOC_ARM_LDR_IMM
: BFD_RELOC_ARM_LITERAL
: BFD_RELOC_ARM_IN_POOL
: BFD_RELOC_ARM_OFFSET_IMM8
: BFD_RELOC_ARM_T32_OFFSET_U8
: BFD_RELOC_ARM_T32_OFFSET_IMM
: BFD_RELOC_ARM_HWLITERAL
: BFD_RELOC_ARM_THUMB_ADD
: BFD_RELOC_ARM_THUMB_IMM
: BFD_RELOC_ARM_THUMB_SHIFT

  These relocs are only used within the ARM assembler. They are not (at present) written to any object files.

: BFD_RELOC_SH_PCDISP8BY2
: BFD_RELOC_SH_PCDISP12BY2
: BFD_RELOC_SH_IMM3
: BFD_RELOC_SH_IMM3U
: BFD_RELOC_SH_DISP12
: BFD_RELOC_SH_DISP12BY2
: BFD_RELOC_SH_DISP12BY4
: BFD_RELOC_SH_DISP12BY8
: BFD_RELOC_SH_DISP20
: BFD_RELOC_SH_DISP20BY8
: BFD_RELOC_SH_IMM4
: BFD_RELOC_SH_IMM4BY2
: BFD_RELOC_SH_IMM4BY4
: BFD_RELOC_SH_IMM8
: BFD_RELOC_SH_IMM8BY2
: BFD_RELOC_SH_IMM8BY4
: BFD_RELOC_SH_PCRELIMM8BY2
: BFD_RELOC_SH_PCRELIMM8BY4
: BFD_RELOC_SH_SWITCH16
: BFD_RELOC_SH_SWITCH32
: BFD_RELOC_SH_USES
: BFD_RELOC_SH_COUNT
: BFD_RELOC_SH_ALIGN
: BFD_RELOC_SH_CODE
: BFD_RELOC_SH_DATA
: BFD_RELOC_SH_LABEL
: BFD_RELOC_SH_LOOP_START
: BFD_RELOC_SH_LOOP_END
: BFD_RELOC_SH_COPY
: BFD_RELOC_SH_GLOB_DAT
: BFD_RELOC_SH_JMP_SLOT
: BFD_RELOC_SH_RELATIVE
: BFD_RELOC_SH_GOTPC
: BFD_RELOC_SH_GOT_LOW16
: BFD_RELOC_SH_GOT_MEDLOW16
: BFD_RELOC_SH_GOT_MEDHI16
: BFD_RELOC_SH_GOT_HI16
: BFD_RELOC_SH_GOTPLT_LOW16
: BFD_RELOC_SH_GOTPLT_MEDLOW16
: BFD_RELOC_SH_GOTPLT_MEDHI16
: BFD_RELOC_SH_GOTPLT_HI16
: BFD_RELOC_SH_PLT_LOW16
: BFD_RELOC_SH_PLT_MEDLOW16
: BFD_RELOC_SH_PLT_MEDHI16
: BFD_RELOC_SH_PLT_HI16
: BFD_RELOC_SH_GOTOFF_LOW16
: BFD_RELOC_SH_GOTOFF_MEDLOW16
: BFD_RELOC_SH_GOTOFF_MEDHI16
: BFD_RELOC_SH_GOTOFF_HI16
: BFD_RELOC_SH_GOTPC_LOW16
: BFD_RELOC_SH_GOTPC_MEDLOW16
: BFD_RELOC_SH_GOTPC_MEDHI16
: BFD_RELOC_SH_GOTPC_HI16
: BFD_RELOC_SH_COPY64
: BFD_RELOC_SH_GLOB_DAT64
: BFD_RELOC_SH_JMP_SLOT64
: BFD_RELOC_SH_RELATIVE64
: BFD_RELOC_SH_GOT10BY4
: BFD_RELOC_SH_GOT10BY8
: BFD_RELOC_SH_GOTPLT10BY4
: BFD_RELOC_SH_GOTPLT10BY8
: BFD_RELOC_SH_GOTPLT32
: BFD_RELOC_SH_SHMEDIA_CODE
: BFD_RELOC_SH_IMMU5
: BFD_RELOC_SH_IMMS6
: BFD_RELOC_SH_IMMS6BY32
: BFD_RELOC_SH_IMMU6
: BFD_RELOC_SH_IMMS10
: BFD_RELOC_SH_IMMS10BY2
: BFD_RELOC_SH_IMMS10BY4
: BFD_RELOC_SH_IMMS10BY8
: BFD_RELOC_SH_IMMS16
: BFD_RELOC_SH_IMMU16
: BFD_RELOC_SH_IMM_LOW16
: BFD_RELOC_SH_IMM_LOW16_PCREL
: BFD_RELOC_SH_IMM_MEDLOW16
: BFD_RELOC_SH_IMM_MEDLOW16_PCREL
: BFD_RELOC_SH_IMM_MEDHI16
: BFD_RELOC_SH_IMM_MEDHI16_PCREL
: BFD_RELOC_SH_IMM_HI16
: BFD_RELOC_SH_IMM_HI16_PCREL
: BFD_RELOC_SH_PT_16
: BFD_RELOC_SH_TLS_GD_32
: BFD_RELOC_SH_TLS_LD_32
: BFD_RELOC_SH_TLS_LDO_32
: BFD_RELOC_SH_TLS_IE_32
: BFD_RELOC_SH_TLS_LE_32
: BFD_RELOC_SH_TLS_DTPMOD32
: BFD_RELOC_SH_TLS_DTPOFF32
: BFD_RELOC_SH_TLS_TPOFF32
: BFD_RELOC_SH_GOT20
: BFD_RELOC_SH_GOTOFF20
: BFD_RELOC_SH_GOTFUNCDESC
: BFD_RELOC_SH_GOTFUNCDESC20
: BFD_RELOC_SH_GOTOFFFUNCDESC
: BFD_RELOC_SH_GOTOFFFUNCDESC20
: BFD_RELOC_SH_FUNCDESC

  Renesas / SuperH SH relocs. Not all of these appear in object files.

: BFD_RELOC_ARC_NONE
: BFD_RELOC_ARC_8
: BFD_RELOC_ARC_16
: BFD_RELOC_ARC_24
: BFD_RELOC_ARC_32
: BFD_RELOC_ARC_N8
: BFD_RELOC_ARC_N16
: BFD_RELOC_ARC_N24
: BFD_RELOC_ARC_N32
: BFD_RELOC_ARC_SDA
: BFD_RELOC_ARC_SECTOFF
: BFD_RELOC_ARC_S21H_PCREL
: BFD_RELOC_ARC_S21W_PCREL
: BFD_RELOC_ARC_S25H_PCREL
: BFD_RELOC_ARC_S25W_PCREL
: BFD_RELOC_ARC_SDA32
: BFD_RELOC_ARC_SDA_LDST
: BFD_RELOC_ARC_SDA_LDST1
: BFD_RELOC_ARC_SDA_LDST2
: BFD_RELOC_ARC_SDA16_LD
: BFD_RELOC_ARC_SDA16_LD1
: BFD_RELOC_ARC_SDA16_LD2
: BFD_RELOC_ARC_S13_PCREL
: BFD_RELOC_ARC_W
: BFD_RELOC_ARC_32_ME
: BFD_RELOC_ARC_32_ME_S
: BFD_RELOC_ARC_N32_ME
: BFD_RELOC_ARC_SECTOFF_ME
: BFD_RELOC_ARC_SDA32_ME
: BFD_RELOC_ARC_W_ME
: BFD_RELOC_AC_SECTOFF_U8
: BFD_RELOC_AC_SECTOFF_U8_1
: BFD_RELOC_AC_SECTOFF_U8_2
: BFD_RELOC_AC_SECTOFF_S9
: BFD_RELOC_AC_SECTOFF_S9_1
: BFD_RELOC_AC_SECTOFF_S9_2
: BFD_RELOC_ARC_SECTOFF_ME_1
: BFD_RELOC_ARC_SECTOFF_ME_2
: BFD_RELOC_ARC_SECTOFF_1
: BFD_RELOC_ARC_SECTOFF_2
: BFD_RELOC_ARC_SDA_12
: BFD_RELOC_ARC_SDA16_ST2
: BFD_RELOC_ARC_32_PCREL
: BFD_RELOC_ARC_PC32
: BFD_RELOC_ARC_GOT32
: BFD_RELOC_ARC_GOTPC32
: BFD_RELOC_ARC_PLT32
: BFD_RELOC_ARC_COPY
: BFD_RELOC_ARC_GLOB_DAT
: BFD_RELOC_ARC_JMP_SLOT
: BFD_RELOC_ARC_RELATIVE
: BFD_RELOC_ARC_GOTOFF
: BFD_RELOC_ARC_GOTPC
: BFD_RELOC_ARC_S21W_PCREL_PLT
: BFD_RELOC_ARC_S25H_PCREL_PLT
: BFD_RELOC_ARC_TLS_DTPMOD
: BFD_RELOC_ARC_TLS_TPOFF
: BFD_RELOC_ARC_TLS_GD_GOT
: BFD_RELOC_ARC_TLS_GD_LD
: BFD_RELOC_ARC_TLS_GD_CALL
: BFD_RELOC_ARC_TLS_IE_GOT
: BFD_RELOC_ARC_TLS_DTPOFF
: BFD_RELOC_ARC_TLS_DTPOFF_S9
: BFD_RELOC_ARC_TLS_LE_S9
: BFD_RELOC_ARC_TLS_LE_32
: BFD_RELOC_ARC_S25W_PCREL_PLT
: BFD_RELOC_ARC_S21H_PCREL_PLT
: BFD_RELOC_ARC_NPS_CMEM16
: BFD_RELOC_ARC_JLI_SECTOFF

  ARC relocs.

: BFD_RELOC_BFIN_16_IMM

  ADI Blackfin 16 bit immediate absolute reloc.

: BFD_RELOC_BFIN_16_HIGH

  ADI Blackfin 16 bit immediate absolute reloc higher 16 bits.

: BFD_RELOC_BFIN_4_PCREL

  ADI Blackfin ’a’ part of LSETUP.

: BFD_RELOC_BFIN_5_PCREL

  ADI Blackfin.

: BFD_RELOC_BFIN_16_LOW

  ADI Blackfin 16 bit immediate absolute reloc lower 16 bits.

: BFD_RELOC_BFIN_10_PCREL

  ADI Blackfin.

: BFD_RELOC_BFIN_11_PCREL

  ADI Blackfin ’b’ part of LSETUP.

: BFD_RELOC_BFIN_12_PCREL_JUMP

  ADI Blackfin.

: BFD_RELOC_BFIN_12_PCREL_JUMP_S

  ADI Blackfin Short jump, pcrel.

: BFD_RELOC_BFIN_24_PCREL_CALL_X

  ADI Blackfin Call.x not implemented.

: BFD_RELOC_BFIN_24_PCREL_JUMP_L

  ADI Blackfin Long Jump pcrel.

: BFD_RELOC_BFIN_GOT17M4
: BFD_RELOC_BFIN_GOTHI
: BFD_RELOC_BFIN_GOTLO
: BFD_RELOC_BFIN_FUNCDESC
: BFD_RELOC_BFIN_FUNCDESC_GOT17M4
: BFD_RELOC_BFIN_FUNCDESC_GOTHI
: BFD_RELOC_BFIN_FUNCDESC_GOTLO
: BFD_RELOC_BFIN_FUNCDESC_VALUE
: BFD_RELOC_BFIN_FUNCDESC_GOTOFF17M4
: BFD_RELOC_BFIN_FUNCDESC_GOTOFFHI
: BFD_RELOC_BFIN_FUNCDESC_GOTOFFLO
: BFD_RELOC_BFIN_GOTOFF17M4
: BFD_RELOC_BFIN_GOTOFFHI
: BFD_RELOC_BFIN_GOTOFFLO

  ADI Blackfin FD-PIC relocations.

: BFD_RELOC_BFIN_GOT

  ADI Blackfin GOT relocation.

: BFD_RELOC_BFIN_PLTPC

  ADI Blackfin PLTPC relocation.

: BFD_ARELOC_BFIN_PUSH

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_CONST

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_ADD

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_SUB

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_MULT

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_DIV

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_MOD

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_LSHIFT

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_RSHIFT

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_AND

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_OR

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_XOR

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_LAND

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_LOR

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_LEN

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_NEG

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_COMP

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_PAGE

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_HWPAGE

  ADI Blackfin arithmetic relocation.

: BFD_ARELOC_BFIN_ADDR

  ADI Blackfin arithmetic relocation.

: BFD_RELOC_D10V_10_PCREL_R

  Mitsubishi D10V relocs. This is a 10-bit reloc with the right 2 bits assumed to be 0.

: BFD_RELOC_D10V_10_PCREL_L

  Mitsubishi D10V relocs. This is a 10-bit reloc with the right 2 bits assumed to be 0. This is the same as the previous reloc except it is in the left container, i.e., shifted left 15 bits.

: BFD_RELOC_D10V_18

  This is an 18-bit reloc with the right 2 bits assumed to be 0.

: BFD_RELOC_D10V_18_PCREL

  This is an 18-bit reloc with the right 2 bits assumed to be 0.

: BFD_RELOC_D30V_6

  Mitsubishi D30V relocs. This is a 6-bit absolute reloc.

: BFD_RELOC_D30V_9_PCREL

  This is a 6-bit pc-relative reloc with the right 3 bits assumed to be 0.

: BFD_RELOC_D30V_9_PCREL_R

  This is a 6-bit pc-relative reloc with the right 3 bits assumed to be 0. Same as the previous reloc but on the right side of the container.

: BFD_RELOC_D30V_15

  This is a 12-bit absolute reloc with the right 3 bitsassumed to be 0.

: BFD_RELOC_D30V_15_PCREL

  This is a 12-bit pc-relative reloc with the right 3 bits assumed to be 0.

: BFD_RELOC_D30V_15_PCREL_R

  This is a 12-bit pc-relative reloc with the right 3 bits assumed to be 0. Same as the previous reloc but on the right side of the container.

: BFD_RELOC_D30V_21

  This is an 18-bit absolute reloc with the right 3 bits assumed to be 0.

: BFD_RELOC_D30V_21_PCREL

  This is an 18-bit pc-relative reloc with the right 3 bits assumed to be 0.

: BFD_RELOC_D30V_21_PCREL_R

  This is an 18-bit pc-relative reloc with the right 3 bits assumed to be 0. Same as the previous reloc but on the right side of the container.

: BFD_RELOC_D30V_32

  This is a 32-bit absolute reloc.

: BFD_RELOC_D30V_32_PCREL

  This is a 32-bit pc-relative reloc.

: BFD_RELOC_DLX_HI16_S

  DLX relocs

: BFD_RELOC_DLX_LO16

  DLX relocs

: BFD_RELOC_DLX_JMP26

  DLX relocs

: BFD_RELOC_M32C_HI8
: BFD_RELOC_M32C_RL_JUMP
: BFD_RELOC_M32C_RL_1ADDR
: BFD_RELOC_M32C_RL_2ADDR

  Renesas M16C/M32C Relocations.

: BFD_RELOC_M32R_24

  Renesas M32R (formerly Mitsubishi M32R) relocs. This is a 24 bit absolute address.

: BFD_RELOC_M32R_10_PCREL

  This is a 10-bit pc-relative reloc with the right 2 bits assumed to be 0.

: BFD_RELOC_M32R_18_PCREL

  This is an 18-bit reloc with the right 2 bits assumed to be 0.

: BFD_RELOC_M32R_26_PCREL

  This is a 26-bit reloc with the right 2 bits assumed to be 0.

: BFD_RELOC_M32R_HI16_ULO

  This is a 16-bit reloc containing the high 16 bits of an address used when the lower 16 bits are treated as unsigned.

: BFD_RELOC_M32R_HI16_SLO

  This is a 16-bit reloc containing the high 16 bits of an address used when the lower 16 bits are treated as signed.

: BFD_RELOC_M32R_LO16

  This is a 16-bit reloc containing the lower 16 bits of an address.

: BFD_RELOC_M32R_SDA16

  This is a 16-bit reloc containing the small data area offset for use in add3, load, and store instructions.

: BFD_RELOC_M32R_GOT24
: BFD_RELOC_M32R_26_PLTREL
: BFD_RELOC_M32R_COPY
: BFD_RELOC_M32R_GLOB_DAT
: BFD_RELOC_M32R_JMP_SLOT
: BFD_RELOC_M32R_RELATIVE
: BFD_RELOC_M32R_GOTOFF
: BFD_RELOC_M32R_GOTOFF_HI_ULO
: BFD_RELOC_M32R_GOTOFF_HI_SLO
: BFD_RELOC_M32R_GOTOFF_LO
: BFD_RELOC_M32R_GOTPC24
: BFD_RELOC_M32R_GOT16_HI_ULO
: BFD_RELOC_M32R_GOT16_HI_SLO
: BFD_RELOC_M32R_GOT16_LO
: BFD_RELOC_M32R_GOTPC_HI_ULO
: BFD_RELOC_M32R_GOTPC_HI_SLO
: BFD_RELOC_M32R_GOTPC_LO

  For PIC.

: BFD_RELOC_NDS32_20

  NDS32 relocs. This is a 20 bit absolute address.

: BFD_RELOC_NDS32_9_PCREL

  This is a 9-bit pc-relative reloc with the right 1 bit assumed to be 0.

: BFD_RELOC_NDS32_WORD_9_PCREL

  This is a 9-bit pc-relative reloc with the right 1 bit assumed to be 0.

: BFD_RELOC_NDS32_15_PCREL

  This is an 15-bit reloc with the right 1 bit assumed to be 0.

: BFD_RELOC_NDS32_17_PCREL

  This is an 17-bit reloc with the right 1 bit assumed to be 0.

: BFD_RELOC_NDS32_25_PCREL

  This is a 25-bit reloc with the right 1 bit assumed to be 0.

: BFD_RELOC_NDS32_HI20

  This is a 20-bit reloc containing the high 20 bits of an address used with the lower 12 bits

: BFD_RELOC_NDS32_LO12S3

  This is a 12-bit reloc containing the lower 12 bits of an address then shift right by 3. This is used with ldi,sdi...

: BFD_RELOC_NDS32_LO12S2

  This is a 12-bit reloc containing the lower 12 bits of an address then shift left by 2. This is used with lwi,swi...

: BFD_RELOC_NDS32_LO12S1

  This is a 12-bit reloc containing the lower 12 bits of an address then shift left by 1. This is used with lhi,shi...

: BFD_RELOC_NDS32_LO12S0

  This is a 12-bit reloc containing the lower 12 bits of an address then shift left by 0. This is used with lbisbi...

: BFD_RELOC_NDS32_LO12S0_ORI

  This is a 12-bit reloc containing the lower 12 bits of an address then shift left by 0. This is only used with branch relaxations

: BFD_RELOC_NDS32_SDA15S3

  This is a 15-bit reloc containing the small data area 18-bit signed offset and shift left by 3 for use in ldi, sdi...

: BFD_RELOC_NDS32_SDA15S2

  This is a 15-bit reloc containing the small data area 17-bit signed offset and shift left by 2 for use in lwi, swi...

: BFD_RELOC_NDS32_SDA15S1

  This is a 15-bit reloc containing the small data area 16-bit signed offset and shift left by 1 for use in lhi, shi...

: BFD_RELOC_NDS32_SDA15S0

  This is a 15-bit reloc containing the small data area 15-bit signed offset and shift left by 0 for use in lbi, sbi...

: BFD_RELOC_NDS32_SDA16S3

  This is a 16-bit reloc containing the small data area 16-bit signed offset and shift left by 3

: BFD_RELOC_NDS32_SDA17S2

  This is a 17-bit reloc containing the small data area 17-bit signed offset and shift left by 2 for use in lwi.gp, swi.gp...

: BFD_RELOC_NDS32_SDA18S1

  This is a 18-bit reloc containing the small data area 18-bit signed offset and shift left by 1 for use in lhi.gp, shi.gp...

: BFD_RELOC_NDS32_SDA19S0

  This is a 19-bit reloc containing the small data area 19-bit signed offset and shift left by 0 for use in lbi.gp, sbi.gp...

: BFD_RELOC_NDS32_GOT20
: BFD_RELOC_NDS32_9_PLTREL
: BFD_RELOC_NDS32_25_PLTREL
: BFD_RELOC_NDS32_COPY
: BFD_RELOC_NDS32_GLOB_DAT
: BFD_RELOC_NDS32_JMP_SLOT
: BFD_RELOC_NDS32_RELATIVE
: BFD_RELOC_NDS32_GOTOFF
: BFD_RELOC_NDS32_GOTOFF_HI20
: BFD_RELOC_NDS32_GOTOFF_LO12
: BFD_RELOC_NDS32_GOTPC20
: BFD_RELOC_NDS32_GOT_HI20
: BFD_RELOC_NDS32_GOT_LO12
: BFD_RELOC_NDS32_GOTPC_HI20
: BFD_RELOC_NDS32_GOTPC_LO12

  for PIC

: BFD_RELOC_NDS32_INSN16
: BFD_RELOC_NDS32_LABEL
: BFD_RELOC_NDS32_LONGCALL1
: BFD_RELOC_NDS32_LONGCALL2
: BFD_RELOC_NDS32_LONGCALL3
: BFD_RELOC_NDS32_LONGJUMP1
: BFD_RELOC_NDS32_LONGJUMP2
: BFD_RELOC_NDS32_LONGJUMP3
: BFD_RELOC_NDS32_LOADSTORE
: BFD_RELOC_NDS32_9_FIXED
: BFD_RELOC_NDS32_15_FIXED
: BFD_RELOC_NDS32_17_FIXED
: BFD_RELOC_NDS32_25_FIXED
: BFD_RELOC_NDS32_LONGCALL4
: BFD_RELOC_NDS32_LONGCALL5
: BFD_RELOC_NDS32_LONGCALL6
: BFD_RELOC_NDS32_LONGJUMP4
: BFD_RELOC_NDS32_LONGJUMP5
: BFD_RELOC_NDS32_LONGJUMP6
: BFD_RELOC_NDS32_LONGJUMP7

  for relax

: BFD_RELOC_NDS32_PLTREL_HI20
: BFD_RELOC_NDS32_PLTREL_LO12
: BFD_RELOC_NDS32_PLT_GOTREL_HI20
: BFD_RELOC_NDS32_PLT_GOTREL_LO12

  for PIC

: BFD_RELOC_NDS32_SDA12S2_DP
: BFD_RELOC_NDS32_SDA12S2_SP
: BFD_RELOC_NDS32_LO12S2_DP
: BFD_RELOC_NDS32_LO12S2_SP

  for floating point

: BFD_RELOC_NDS32_DWARF2_OP1
: BFD_RELOC_NDS32_DWARF2_OP2
: BFD_RELOC_NDS32_DWARF2_LEB

  for dwarf2 debug_line.

: BFD_RELOC_NDS32_UPDATE_TA

  for eliminate 16-bit instructions

: BFD_RELOC_NDS32_PLT_GOTREL_LO20
: BFD_RELOC_NDS32_PLT_GOTREL_LO15
: BFD_RELOC_NDS32_PLT_GOTREL_LO19
: BFD_RELOC_NDS32_GOT_LO15
: BFD_RELOC_NDS32_GOT_LO19
: BFD_RELOC_NDS32_GOTOFF_LO15
: BFD_RELOC_NDS32_GOTOFF_LO19
: BFD_RELOC_NDS32_GOT15S2
: BFD_RELOC_NDS32_GOT17S2

  for PIC object relaxation

: BFD_RELOC_NDS32_5

  NDS32 relocs. This is a 5 bit absolute address.

: BFD_RELOC_NDS32_10_UPCREL

  This is a 10-bit unsigned pc-relative reloc with the right 1 bit assumed to be 0.

: BFD_RELOC_NDS32_SDA_FP7U2_RELA

  If fp were omitted, fp can used as another gp.

: BFD_RELOC_NDS32_RELAX_ENTRY
: BFD_RELOC_NDS32_GOT_SUFF
: BFD_RELOC_NDS32_GOTOFF_SUFF
: BFD_RELOC_NDS32_PLT_GOT_SUFF
: BFD_RELOC_NDS32_MULCALL_SUFF
: BFD_RELOC_NDS32_PTR
: BFD_RELOC_NDS32_PTR_COUNT
: BFD_RELOC_NDS32_PTR_RESOLVED
: BFD_RELOC_NDS32_PLTBLOCK
: BFD_RELOC_NDS32_RELAX_REGION_BEGIN
: BFD_RELOC_NDS32_RELAX_REGION_END
: BFD_RELOC_NDS32_MINUEND
: BFD_RELOC_NDS32_SUBTRAHEND
: BFD_RELOC_NDS32_DIFF8
: BFD_RELOC_NDS32_DIFF16
: BFD_RELOC_NDS32_DIFF32
: BFD_RELOC_NDS32_DIFF_ULEB128
: BFD_RELOC_NDS32_EMPTY

  relaxation relative relocation types

: BFD_RELOC_NDS32_25_ABS

  This is a 25 bit absolute address.

: BFD_RELOC_NDS32_DATA
: BFD_RELOC_NDS32_TRAN
: BFD_RELOC_NDS32_17IFC_PCREL
: BFD_RELOC_NDS32_10IFCU_PCREL

  For ex9 and ifc using.

: BFD_RELOC_NDS32_TPOFF
: BFD_RELOC_NDS32_TLS_LE_HI20
: BFD_RELOC_NDS32_TLS_LE_LO12
: BFD_RELOC_NDS32_TLS_LE_ADD
: BFD_RELOC_NDS32_TLS_LE_LS
: BFD_RELOC_NDS32_GOTTPOFF
: BFD_RELOC_NDS32_TLS_IE_HI20
: BFD_RELOC_NDS32_TLS_IE_LO12S2
: BFD_RELOC_NDS32_TLS_TPOFF
: BFD_RELOC_NDS32_TLS_LE_20
: BFD_RELOC_NDS32_TLS_LE_15S0
: BFD_RELOC_NDS32_TLS_LE_15S1
: BFD_RELOC_NDS32_TLS_LE_15S2

  For TLS.

: BFD_RELOC_V850_9_PCREL

  This is a 9-bit reloc

: BFD_RELOC_V850_22_PCREL

  This is a 22-bit reloc

: BFD_RELOC_V850_SDA_16_16_OFFSET

  This is a 16 bit offset from the short data area pointer.

: BFD_RELOC_V850_SDA_15_16_OFFSET

  This is a 16 bit offset (of which only 15 bits are used) from the short data area pointer.

: BFD_RELOC_V850_ZDA_16_16_OFFSET

  This is a 16 bit offset from the zero data area pointer.

: BFD_RELOC_V850_ZDA_15_16_OFFSET

  This is a 16 bit offset (of which only 15 bits are used) from the zero data area pointer.

: BFD_RELOC_V850_TDA_6_8_OFFSET

  This is an 8 bit offset (of which only 6 bits are used) from the tiny data area pointer.

: BFD_RELOC_V850_TDA_7_8_OFFSET

  This is an 8bit offset (of which only 7 bits are used) from the tiny data area pointer.

: BFD_RELOC_V850_TDA_7_7_OFFSET

  This is a 7 bit offset from the tiny data area pointer.

: BFD_RELOC_V850_TDA_16_16_OFFSET

  This is a 16 bit offset from the tiny data area pointer.

: BFD_RELOC_V850_TDA_4_5_OFFSET

  This is a 5 bit offset (of which only 4 bits are used) from the tiny data area pointer.

: BFD_RELOC_V850_TDA_4_4_OFFSET

  This is a 4 bit offset from the tiny data area pointer.

: BFD_RELOC_V850_SDA_16_16_SPLIT_OFFSET

  This is a 16 bit offset from the short data area pointer, with the bits placed non-contiguously in the instruction.

: BFD_RELOC_V850_ZDA_16_16_SPLIT_OFFSET

  This is a 16 bit offset from the zero data area pointer, with the bits placed non-contiguously in the instruction.

: BFD_RELOC_V850_CALLT_6_7_OFFSET

  This is a 6 bit offset from the call table base pointer.

: BFD_RELOC_V850_CALLT_16_16_OFFSET

  This is a 16 bit offset from the call table base pointer.

: BFD_RELOC_V850_LONGCALL

  Used for relaxing indirect function calls.

: BFD_RELOC_V850_LONGJUMP

  Used for relaxing indirect jumps.

: BFD_RELOC_V850_ALIGN

  Used to maintain alignment whilst relaxing.

: BFD_RELOC_V850_LO16_SPLIT_OFFSET

  This is a variation of BFD_RELOC_LO16 that can be used in v850e ld.bu instructions.

: BFD_RELOC_V850_16_PCREL

  This is a 16-bit reloc.

: BFD_RELOC_V850_17_PCREL

  This is a 17-bit reloc.

: BFD_RELOC_V850_23

  This is a 23-bit reloc.

: BFD_RELOC_V850_32_PCREL

  This is a 32-bit reloc.

: BFD_RELOC_V850_32_ABS

  This is a 32-bit reloc.

: BFD_RELOC_V850_16_SPLIT_OFFSET

  This is a 16-bit reloc.

: BFD_RELOC_V850_16_S1

  This is a 16-bit reloc.

: BFD_RELOC_V850_LO16_S1

  Low 16 bits. 16 bit shifted by 1.

: BFD_RELOC_V850_CALLT_15_16_OFFSET

  This is a 16 bit offset from the call table base pointer.

: BFD_RELOC_V850_32_GOTPCREL

  DSO relocations.

: BFD_RELOC_V850_16_GOT

  DSO relocations.

: BFD_RELOC_V850_32_GOT

  DSO relocations.

: BFD_RELOC_V850_22_PLT_PCREL

  DSO relocations.

: BFD_RELOC_V850_32_PLT_PCREL

  DSO relocations.

: BFD_RELOC_V850_COPY

  DSO relocations.

: BFD_RELOC_V850_GLOB_DAT

  DSO relocations.

: BFD_RELOC_V850_JMP_SLOT

  DSO relocations.

: BFD_RELOC_V850_RELATIVE

  DSO relocations.

: BFD_RELOC_V850_16_GOTOFF

  DSO relocations.

: BFD_RELOC_V850_32_GOTOFF

  DSO relocations.

: BFD_RELOC_V850_CODE

  start code.

: BFD_RELOC_V850_DATA

  start data in text.

: BFD_RELOC_TIC30_LDP

  This is a 8bit DP reloc for the tms320c30, where the most significant 8 bits of a 24 bit word are placed into the least significant 8 bits of the opcode.

: BFD_RELOC_TIC54X_PARTLS7

  This is a 7bit reloc for the tms320c54x, where the least significant 7 bits of a 16 bit word are placed into the least significant 7 bits of the opcode.

: BFD_RELOC_TIC54X_PARTMS9

  This is a 9bit DP reloc for the tms320c54x, where the most significant 9 bits of a 16 bit word are placed into the least significant 9 bits of the opcode.

: BFD_RELOC_TIC54X_23

  This is an extended address 23-bit reloc for the tms320c54x.

: BFD_RELOC_TIC54X_16_OF_23

  This is a 16-bit reloc for the tms320c54x, where the least significant 16 bits of a 23-bit extended address are placed into the opcode.

: BFD_RELOC_TIC54X_MS7_OF_23

  This is a reloc for the tms320c54x, where the most significant 7 bits of a 23-bit extended address are placed into the opcode.

: BFD_RELOC_C6000_PCR_S21
: BFD_RELOC_C6000_PCR_S12
: BFD_RELOC_C6000_PCR_S10
: BFD_RELOC_C6000_PCR_S7
: BFD_RELOC_C6000_ABS_S16
: BFD_RELOC_C6000_ABS_L16
: BFD_RELOC_C6000_ABS_H16
: BFD_RELOC_C6000_SBR_U15_B
: BFD_RELOC_C6000_SBR_U15_H
: BFD_RELOC_C6000_SBR_U15_W
: BFD_RELOC_C6000_SBR_S16
: BFD_RELOC_C6000_SBR_L16_B
: BFD_RELOC_C6000_SBR_L16_H
: BFD_RELOC_C6000_SBR_L16_W
: BFD_RELOC_C6000_SBR_H16_B
: BFD_RELOC_C6000_SBR_H16_H
: BFD_RELOC_C6000_SBR_H16_W
: BFD_RELOC_C6000_SBR_GOT_U15_W
: BFD_RELOC_C6000_SBR_GOT_L16_W
: BFD_RELOC_C6000_SBR_GOT_H16_W
: BFD_RELOC_C6000_DSBT_INDEX
: BFD_RELOC_C6000_PREL31
: BFD_RELOC_C6000_COPY
: BFD_RELOC_C6000_JUMP_SLOT
: BFD_RELOC_C6000_EHTYPE
: BFD_RELOC_C6000_PCR_H16
: BFD_RELOC_C6000_PCR_L16
: BFD_RELOC_C6000_ALIGN
: BFD_RELOC_C6000_FPHEAD
: BFD_RELOC_C6000_NOCMP

  TMS320C6000 relocations.

: BFD_RELOC_FR30_48

  This is a 48 bit reloc for the FR30 that stores 32 bits.

: BFD_RELOC_FR30_20

  This is a 32 bit reloc for the FR30 that stores 20 bits split up into two sections.

: BFD_RELOC_FR30_6_IN_4

  This is a 16 bit reloc for the FR30 that stores a 6 bit word offset in 4 bits.

: BFD_RELOC_FR30_8_IN_8

  This is a 16 bit reloc for the FR30 that stores an 8 bit byte offset into 8 bits.

: BFD_RELOC_FR30_9_IN_8

  This is a 16 bit reloc for the FR30 that stores a 9 bit short offset into 8 bits.

: BFD_RELOC_FR30_10_IN_8

  This is a 16 bit reloc for the FR30 that stores a 10 bit word offset into 8 bits.

: BFD_RELOC_FR30_9_PCREL

  This is a 16 bit reloc for the FR30 that stores a 9 bit pc relative short offset into 8 bits.

: BFD_RELOC_FR30_12_PCREL

  This is a 16 bit reloc for the FR30 that stores a 12 bit pc relative short offset into 11 bits.

: BFD_RELOC_MCORE_PCREL_IMM8BY4
: BFD_RELOC_MCORE_PCREL_IMM11BY2
: BFD_RELOC_MCORE_PCREL_IMM4BY2
: BFD_RELOC_MCORE_PCREL_32
: BFD_RELOC_MCORE_PCREL_JSR_IMM11BY2
: BFD_RELOC_MCORE_RVA

  Motorola Mcore relocations.

: BFD_RELOC_MEP_8
: BFD_RELOC_MEP_16
: BFD_RELOC_MEP_32
: BFD_RELOC_MEP_PCREL8A2
: BFD_RELOC_MEP_PCREL12A2
: BFD_RELOC_MEP_PCREL17A2
: BFD_RELOC_MEP_PCREL24A2
: BFD_RELOC_MEP_PCABS24A2
: BFD_RELOC_MEP_LOW16
: BFD_RELOC_MEP_HI16U
: BFD_RELOC_MEP_HI16S
: BFD_RELOC_MEP_GPREL
: BFD_RELOC_MEP_TPREL
: BFD_RELOC_MEP_TPREL7
: BFD_RELOC_MEP_TPREL7A2
: BFD_RELOC_MEP_TPREL7A4
: BFD_RELOC_MEP_UIMM24
: BFD_RELOC_MEP_ADDR24A4
: BFD_RELOC_MEP_GNU_VTINHERIT
: BFD_RELOC_MEP_GNU_VTENTRY

  Toshiba Media Processor Relocations.

: BFD_RELOC_METAG_HIADDR16
: BFD_RELOC_METAG_LOADDR16
: BFD_RELOC_METAG_RELBRANCH
: BFD_RELOC_METAG_GETSETOFF
: BFD_RELOC_METAG_HIOG
: BFD_RELOC_METAG_LOOG
: BFD_RELOC_METAG_REL8
: BFD_RELOC_METAG_REL16
: BFD_RELOC_METAG_HI16_GOTOFF
: BFD_RELOC_METAG_LO16_GOTOFF
: BFD_RELOC_METAG_GETSET_GOTOFF
: BFD_RELOC_METAG_GETSET_GOT
: BFD_RELOC_METAG_HI16_GOTPC
: BFD_RELOC_METAG_LO16_GOTPC
: BFD_RELOC_METAG_HI16_PLT
: BFD_RELOC_METAG_LO16_PLT
: BFD_RELOC_METAG_RELBRANCH_PLT
: BFD_RELOC_METAG_GOTOFF
: BFD_RELOC_METAG_PLT
: BFD_RELOC_METAG_COPY
: BFD_RELOC_METAG_JMP_SLOT
: BFD_RELOC_METAG_RELATIVE
: BFD_RELOC_METAG_GLOB_DAT
: BFD_RELOC_METAG_TLS_GD
: BFD_RELOC_METAG_TLS_LDM
: BFD_RELOC_METAG_TLS_LDO_HI16
: BFD_RELOC_METAG_TLS_LDO_LO16
: BFD_RELOC_METAG_TLS_LDO
: BFD_RELOC_METAG_TLS_IE
: BFD_RELOC_METAG_TLS_IENONPIC
: BFD_RELOC_METAG_TLS_IENONPIC_HI16
: BFD_RELOC_METAG_TLS_IENONPIC_LO16
: BFD_RELOC_METAG_TLS_TPOFF
: BFD_RELOC_METAG_TLS_DTPMOD
: BFD_RELOC_METAG_TLS_DTPOFF
: BFD_RELOC_METAG_TLS_LE
: BFD_RELOC_METAG_TLS_LE_HI16
: BFD_RELOC_METAG_TLS_LE_LO16

  Imagination Technologies Meta relocations.

: BFD_RELOC_MMIX_GETA
: BFD_RELOC_MMIX_GETA_1
: BFD_RELOC_MMIX_GETA_2
: BFD_RELOC_MMIX_GETA_3

  These are relocations for the GETA instruction.

: BFD_RELOC_MMIX_CBRANCH
: BFD_RELOC_MMIX_CBRANCH_J
: BFD_RELOC_MMIX_CBRANCH_1
: BFD_RELOC_MMIX_CBRANCH_2
: BFD_RELOC_MMIX_CBRANCH_3

  These are relocations for a conditional branch instruction.

: BFD_RELOC_MMIX_PUSHJ
: BFD_RELOC_MMIX_PUSHJ_1
: BFD_RELOC_MMIX_PUSHJ_2
: BFD_RELOC_MMIX_PUSHJ_3
: BFD_RELOC_MMIX_PUSHJ_STUBBABLE

  These are relocations for the PUSHJ instruction.

: BFD_RELOC_MMIX_JMP
: BFD_RELOC_MMIX_JMP_1
: BFD_RELOC_MMIX_JMP_2
: BFD_RELOC_MMIX_JMP_3

  These are relocations for the JMP instruction.

: BFD_RELOC_MMIX_ADDR19

  This is a relocation for a relative address as in a GETA instruction or a branch.

: BFD_RELOC_MMIX_ADDR27

  This is a relocation for a relative address as in a JMP instruction.

: BFD_RELOC_MMIX_REG_OR_BYTE

  This is a relocation for an instruction field that may be a general register or a value 0..255.

: BFD_RELOC_MMIX_REG

  This is a relocation for an instruction field that may be a general register.

: BFD_RELOC_MMIX_BASE_PLUS_OFFSET

  This is a relocation for two instruction fields holding a register and an offset, the equivalent of the relocation.

: BFD_RELOC_MMIX_LOCAL

  This relocation is an assertion that the expression is not allocated as a global register. It does not modify contents.

: BFD_RELOC_AVR_7_PCREL

  This is a 16 bit reloc for the AVR that stores 8 bit pc relative short offset into 7 bits.

: BFD_RELOC_AVR_13_PCREL

  This is a 16 bit reloc for the AVR that stores 13 bit pc relative short offset into 12 bits.

: BFD_RELOC_AVR_16_PM

  This is a 16 bit reloc for the AVR that stores 17 bit value (usually program memory address) into 16 bits.

: BFD_RELOC_AVR_LO8_LDI

  This is a 16 bit reloc for the AVR that stores 8 bit value (usually data memory address) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_HI8_LDI

  This is a 16 bit reloc for the AVR that stores 8 bit value (high 8 bit of data memory address) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_HH8_LDI

  This is a 16 bit reloc for the AVR that stores 8 bit value (most high 8 bit of program memory address) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_MS8_LDI

  This is a 16 bit reloc for the AVR that stores 8 bit value (most high 8 bit of 32 bit value) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_LO8_LDI_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (usually data memory address) into 8 bit immediate value of SUBI insn.

: BFD_RELOC_AVR_HI8_LDI_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (high 8 bit of data memory address) into 8 bit immediate value of SUBI insn.

: BFD_RELOC_AVR_HH8_LDI_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (most high 8 bit of program memory address) into 8 bit immediate value of LDI or SUBI insn.

: BFD_RELOC_AVR_MS8_LDI_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (msb of 32 bit value) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_LO8_LDI_PM

  This is a 16 bit reloc for the AVR that stores 8 bit value (usually command address) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_LO8_LDI_GS

  This is a 16 bit reloc for the AVR that stores 8 bit value (command address) into 8 bit immediate value of LDI insn. If the address is beyond the 128k boundary, the linker inserts a jump stub for this reloc in the lower 128k.

: BFD_RELOC_AVR_HI8_LDI_PM

  This is a 16 bit reloc for the AVR that stores 8 bit value (high 8 bit of command address) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_HI8_LDI_GS

  This is a 16 bit reloc for the AVR that stores 8 bit value (high 8 bit of command address) into 8 bit immediate value of LDI insn. If the address is beyond the 128k boundary, the linker inserts a jump stub for this reloc below 128k.

: BFD_RELOC_AVR_HH8_LDI_PM

  This is a 16 bit reloc for the AVR that stores 8 bit value (most high 8 bit of command address) into 8 bit immediate value of LDI insn.

: BFD_RELOC_AVR_LO8_LDI_PM_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (usually command address) into 8 bit immediate value of SUBI insn.

: BFD_RELOC_AVR_HI8_LDI_PM_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (high 8 bit of 16 bit command address) into 8 bit immediate value of SUBI insn.

: BFD_RELOC_AVR_HH8_LDI_PM_NEG

  This is a 16 bit reloc for the AVR that stores negated 8 bit value (high 6 bit of 22 bit command address) into 8 bit immediate value of SUBI insn.

: BFD_RELOC_AVR_CALL

  This is a 32 bit reloc for the AVR that stores 23 bit value into 22 bits.

: BFD_RELOC_AVR_LDI

  This is a 16 bit reloc for the AVR that stores all needed bits for absolute addressing with ldi with overflow check to linktime

: BFD_RELOC_AVR_6

  This is a 6 bit reloc for the AVR that stores offset for ldd/std instructions

: BFD_RELOC_AVR_6_ADIW

  This is a 6 bit reloc for the AVR that stores offset for adiw/sbiw instructions

: BFD_RELOC_AVR_8_LO

  This is a 8 bit reloc for the AVR that stores bits 0..7 of a symbol in .byte lo8(symbol)

: BFD_RELOC_AVR_8_HI

  This is a 8 bit reloc for the AVR that stores bits 8..15 of a symbol in .byte hi8(symbol)

: BFD_RELOC_AVR_8_HLO

  This is a 8 bit reloc for the AVR that stores bits 16..23 of a symbol in .byte hlo8(symbol)

: BFD_RELOC_AVR_DIFF8
: BFD_RELOC_AVR_DIFF16
: BFD_RELOC_AVR_DIFF32

  AVR relocations to mark the difference of two local symbols. These are only needed to support linker relaxation and can be ignored when not relaxing. The field is set to the value of the difference assuming no relaxation. The relocation encodes the position of the second symbol so the linker can determine whether to adjust the field value.

: BFD_RELOC_AVR_LDS_STS_16

  This is a 7 bit reloc for the AVR that stores SRAM address for 16bit lds and sts instructions supported only tiny core.

: BFD_RELOC_AVR_PORT6

  This is a 6 bit reloc for the AVR that stores an I/O register number for the IN and OUT instructions

: BFD_RELOC_AVR_PORT5

  This is a 5 bit reloc for the AVR that stores an I/O register number for the SBIC, SBIS, SBI and CBI instructions

: BFD_RELOC_RISCV_HI20
: BFD_RELOC_RISCV_PCREL_HI20
: BFD_RELOC_RISCV_PCREL_LO12_I
: BFD_RELOC_RISCV_PCREL_LO12_S
: BFD_RELOC_RISCV_LO12_I
: BFD_RELOC_RISCV_LO12_S
: BFD_RELOC_RISCV_GPREL12_I
: BFD_RELOC_RISCV_GPREL12_S
: BFD_RELOC_RISCV_TPREL_HI20
: BFD_RELOC_RISCV_TPREL_LO12_I
: BFD_RELOC_RISCV_TPREL_LO12_S
: BFD_RELOC_RISCV_TPREL_ADD
: BFD_RELOC_RISCV_CALL
: BFD_RELOC_RISCV_CALL_PLT
: BFD_RELOC_RISCV_ADD8
: BFD_RELOC_RISCV_ADD16
: BFD_RELOC_RISCV_ADD32
: BFD_RELOC_RISCV_ADD64
: BFD_RELOC_RISCV_SUB8
: BFD_RELOC_RISCV_SUB16
: BFD_RELOC_RISCV_SUB32
: BFD_RELOC_RISCV_SUB64
: BFD_RELOC_RISCV_GOT_HI20
: BFD_RELOC_RISCV_TLS_GOT_HI20
: BFD_RELOC_RISCV_TLS_GD_HI20
: BFD_RELOC_RISCV_JMP
: BFD_RELOC_RISCV_TLS_DTPMOD32
: BFD_RELOC_RISCV_TLS_DTPREL32
: BFD_RELOC_RISCV_TLS_DTPMOD64
: BFD_RELOC_RISCV_TLS_DTPREL64
: BFD_RELOC_RISCV_TLS_TPREL32
: BFD_RELOC_RISCV_TLS_TPREL64
: BFD_RELOC_RISCV_ALIGN
: BFD_RELOC_RISCV_RVC_BRANCH
: BFD_RELOC_RISCV_RVC_JUMP
: BFD_RELOC_RISCV_RVC_LUI
: BFD_RELOC_RISCV_GPREL_I
: BFD_RELOC_RISCV_GPREL_S
: BFD_RELOC_RISCV_TPREL_I
: BFD_RELOC_RISCV_TPREL_S
: BFD_RELOC_RISCV_RELAX
: BFD_RELOC_RISCV_CFA
: BFD_RELOC_RISCV_SUB6
: BFD_RELOC_RISCV_SET6
: BFD_RELOC_RISCV_SET8
: BFD_RELOC_RISCV_SET16
: BFD_RELOC_RISCV_SET32
: BFD_RELOC_RISCV_32_PCREL

  RISC-V relocations.

: BFD_RELOC_RL78_NEG8
: BFD_RELOC_RL78_NEG16
: BFD_RELOC_RL78_NEG24
: BFD_RELOC_RL78_NEG32
: BFD_RELOC_RL78_16_OP
: BFD_RELOC_RL78_24_OP
: BFD_RELOC_RL78_32_OP
: BFD_RELOC_RL78_8U
: BFD_RELOC_RL78_16U
: BFD_RELOC_RL78_24U
: BFD_RELOC_RL78_DIR3U_PCREL
: BFD_RELOC_RL78_DIFF
: BFD_RELOC_RL78_GPRELB
: BFD_RELOC_RL78_GPRELW
: BFD_RELOC_RL78_GPRELL
: BFD_RELOC_RL78_SYM
: BFD_RELOC_RL78_OP_SUBTRACT
: BFD_RELOC_RL78_OP_NEG
: BFD_RELOC_RL78_OP_AND
: BFD_RELOC_RL78_OP_SHRA
: BFD_RELOC_RL78_ABS8
: BFD_RELOC_RL78_ABS16
: BFD_RELOC_RL78_ABS16_REV
: BFD_RELOC_RL78_ABS32
: BFD_RELOC_RL78_ABS32_REV
: BFD_RELOC_RL78_ABS16U
: BFD_RELOC_RL78_ABS16UW
: BFD_RELOC_RL78_ABS16UL
: BFD_RELOC_RL78_RELAX
: BFD_RELOC_RL78_HI16
: BFD_RELOC_RL78_HI8
: BFD_RELOC_RL78_LO16
: BFD_RELOC_RL78_CODE
: BFD_RELOC_RL78_SADDR

  Renesas RL78 Relocations.

: BFD_RELOC_RX_NEG8
: BFD_RELOC_RX_NEG16
: BFD_RELOC_RX_NEG24
: BFD_RELOC_RX_NEG32
: BFD_RELOC_RX_16_OP
: BFD_RELOC_RX_24_OP
: BFD_RELOC_RX_32_OP
: BFD_RELOC_RX_8U
: BFD_RELOC_RX_16U
: BFD_RELOC_RX_24U
: BFD_RELOC_RX_DIR3U_PCREL
: BFD_RELOC_RX_DIFF
: BFD_RELOC_RX_GPRELB
: BFD_RELOC_RX_GPRELW
: BFD_RELOC_RX_GPRELL
: BFD_RELOC_RX_SYM
: BFD_RELOC_RX_OP_SUBTRACT
: BFD_RELOC_RX_OP_NEG
: BFD_RELOC_RX_ABS8
: BFD_RELOC_RX_ABS16
: BFD_RELOC_RX_ABS16_REV
: BFD_RELOC_RX_ABS32
: BFD_RELOC_RX_ABS32_REV
: BFD_RELOC_RX_ABS16U
: BFD_RELOC_RX_ABS16UW
: BFD_RELOC_RX_ABS16UL
: BFD_RELOC_RX_RELAX

  Renesas RX Relocations.

: BFD_RELOC_390_12

  Direct 12 bit.

: BFD_RELOC_390_GOT12

  12 bit GOT offset.

: BFD_RELOC_390_PLT32

  32 bit PC relative PLT address.

: BFD_RELOC_390_COPY

  Copy symbol at runtime.

: BFD_RELOC_390_GLOB_DAT

  Create GOT entry.

: BFD_RELOC_390_JMP_SLOT

  Create PLT entry.

: BFD_RELOC_390_RELATIVE

  Adjust by program base.

: BFD_RELOC_390_GOTPC

  32 bit PC relative offset to GOT.

: BFD_RELOC_390_GOT16

  16 bit GOT offset.

: BFD_RELOC_390_PC12DBL

  PC relative 12 bit shifted by 1.

: BFD_RELOC_390_PLT12DBL

  12 bit PC rel. PLT shifted by 1.

: BFD_RELOC_390_PC16DBL

  PC relative 16 bit shifted by 1.

: BFD_RELOC_390_PLT16DBL

  16 bit PC rel. PLT shifted by 1.

: BFD_RELOC_390_PC24DBL

  PC relative 24 bit shifted by 1.

: BFD_RELOC_390_PLT24DBL

  24 bit PC rel. PLT shifted by 1.

: BFD_RELOC_390_PC32DBL

  PC relative 32 bit shifted by 1.

: BFD_RELOC_390_PLT32DBL

  32 bit PC rel. PLT shifted by 1.

: BFD_RELOC_390_GOTPCDBL

  32 bit PC rel. GOT shifted by 1.

: BFD_RELOC_390_GOT64

  64 bit GOT offset.

: BFD_RELOC_390_PLT64

  64 bit PC relative PLT address.

: BFD_RELOC_390_GOTENT

  32 bit rel. offset to GOT entry.

: BFD_RELOC_390_GOTOFF64

  64 bit offset to GOT.

: BFD_RELOC_390_GOTPLT12

  12-bit offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_390_GOTPLT16

  16-bit offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_390_GOTPLT32

  32-bit offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_390_GOTPLT64

  64-bit offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_390_GOTPLTENT

  32-bit rel. offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_390_PLTOFF16

  16-bit rel. offset from the GOT to a PLT entry.

: BFD_RELOC_390_PLTOFF32

  32-bit rel. offset from the GOT to a PLT entry.

: BFD_RELOC_390_PLTOFF64

  64-bit rel. offset from the GOT to a PLT entry.

: BFD_RELOC_390_TLS_LOAD
: BFD_RELOC_390_TLS_GDCALL
: BFD_RELOC_390_TLS_LDCALL
: BFD_RELOC_390_TLS_GD32
: BFD_RELOC_390_TLS_GD64
: BFD_RELOC_390_TLS_GOTIE12
: BFD_RELOC_390_TLS_GOTIE32
: BFD_RELOC_390_TLS_GOTIE64
: BFD_RELOC_390_TLS_LDM32
: BFD_RELOC_390_TLS_LDM64
: BFD_RELOC_390_TLS_IE32
: BFD_RELOC_390_TLS_IE64
: BFD_RELOC_390_TLS_IEENT
: BFD_RELOC_390_TLS_LE32
: BFD_RELOC_390_TLS_LE64
: BFD_RELOC_390_TLS_LDO32
: BFD_RELOC_390_TLS_LDO64
: BFD_RELOC_390_TLS_DTPMOD
: BFD_RELOC_390_TLS_DTPOFF
: BFD_RELOC_390_TLS_TPOFF

  s390 tls relocations.

: BFD_RELOC_390_20
: BFD_RELOC_390_GOT20
: BFD_RELOC_390_GOTPLT20
: BFD_RELOC_390_TLS_GOTIE20

  Long displacement extension.

: BFD_RELOC_390_IRELATIVE

  STT_GNU_IFUNC relocation.

: BFD_RELOC_SCORE_GPREL15

  Score relocations Low 16 bit for load/store

: BFD_RELOC_SCORE_DUMMY2
: BFD_RELOC_SCORE_JMP

  This is a 24-bit reloc with the right 1 bit assumed to be 0

: BFD_RELOC_SCORE_BRANCH

  This is a 19-bit reloc with the right 1 bit assumed to be 0

: BFD_RELOC_SCORE_IMM30

  This is a 32-bit reloc for 48-bit instructions.

: BFD_RELOC_SCORE_IMM32

  This is a 32-bit reloc for 48-bit instructions.

: BFD_RELOC_SCORE16_JMP

  This is a 11-bit reloc with the right 1 bit assumed to be 0

: BFD_RELOC_SCORE16_BRANCH

  This is a 8-bit reloc with the right 1 bit assumed to be 0

: BFD_RELOC_SCORE_BCMP

  This is a 9-bit reloc with the right 1 bit assumed to be 0

: BFD_RELOC_SCORE_GOT15
: BFD_RELOC_SCORE_GOT_LO16
: BFD_RELOC_SCORE_CALL15
: BFD_RELOC_SCORE_DUMMY_HI16

  Undocumented Score relocs

: BFD_RELOC_IP2K_FR9

  Scenix IP2K - 9-bit register number / data address

: BFD_RELOC_IP2K_BANK

  Scenix IP2K - 4-bit register/data bank number

: BFD_RELOC_IP2K_ADDR16CJP

  Scenix IP2K - low 13 bits of instruction word address

: BFD_RELOC_IP2K_PAGE3

  Scenix IP2K - high 3 bits of instruction word address

: BFD_RELOC_IP2K_LO8DATA
: BFD_RELOC_IP2K_HI8DATA
: BFD_RELOC_IP2K_EX8DATA

  Scenix IP2K - ext/low/high 8 bits of data address

: BFD_RELOC_IP2K_LO8INSN
: BFD_RELOC_IP2K_HI8INSN

  Scenix IP2K - low/high 8 bits of instruction word address

: BFD_RELOC_IP2K_PC_SKIP

  Scenix IP2K - even/odd PC modifier to modify snb pcl.0

: BFD_RELOC_IP2K_TEXT

  Scenix IP2K - 16 bit word address in text section.

: BFD_RELOC_IP2K_FR_OFFSET

  Scenix IP2K - 7-bit sp or dp offset

: BFD_RELOC_VPE4KMATH_DATA
: BFD_RELOC_VPE4KMATH_INSN

  Scenix VPE4K coprocessor - data/insn-space addressing

: BFD_RELOC_VTABLE_INHERIT
: BFD_RELOC_VTABLE_ENTRY

  These two relocations are used by the linker to determine which of the entries in a C++ virtual function table are actually used. When the –gc-sections option is given, the linker will zero out the entries that are not used, so that the code for those functions need not be included in the output.

  VTABLE_INHERIT is a zero-space relocation used to describe to the linker the inheritance tree of a C++ virtual function table. The relocation’s symbol should be the parent class’ vtable, and the relocation should be located at the child vtable.

  VTABLE_ENTRY is a zero-space relocation that describes the use of a virtual function table entry. The reloc’s symbol should refer to the table of the class mentioned in the code. Off of that base, an offset describes the entry that is being used. For Rela hosts, this offset is stored in the reloc’s addend. For Rel hosts, we are forced to put this offset in the reloc’s section offset.

: BFD_RELOC_IA64_IMM14
: BFD_RELOC_IA64_IMM22
: BFD_RELOC_IA64_IMM64
: BFD_RELOC_IA64_DIR32MSB
: BFD_RELOC_IA64_DIR32LSB
: BFD_RELOC_IA64_DIR64MSB
: BFD_RELOC_IA64_DIR64LSB
: BFD_RELOC_IA64_GPREL22
: BFD_RELOC_IA64_GPREL64I
: BFD_RELOC_IA64_GPREL32MSB
: BFD_RELOC_IA64_GPREL32LSB
: BFD_RELOC_IA64_GPREL64MSB
: BFD_RELOC_IA64_GPREL64LSB
: BFD_RELOC_IA64_LTOFF22
: BFD_RELOC_IA64_LTOFF64I
: BFD_RELOC_IA64_PLTOFF22
: BFD_RELOC_IA64_PLTOFF64I
: BFD_RELOC_IA64_PLTOFF64MSB
: BFD_RELOC_IA64_PLTOFF64LSB
: BFD_RELOC_IA64_FPTR64I
: BFD_RELOC_IA64_FPTR32MSB
: BFD_RELOC_IA64_FPTR32LSB
: BFD_RELOC_IA64_FPTR64MSB
: BFD_RELOC_IA64_FPTR64LSB
: BFD_RELOC_IA64_PCREL21B
: BFD_RELOC_IA64_PCREL21BI
: BFD_RELOC_IA64_PCREL21M
: BFD_RELOC_IA64_PCREL21F
: BFD_RELOC_IA64_PCREL22
: BFD_RELOC_IA64_PCREL60B
: BFD_RELOC_IA64_PCREL64I
: BFD_RELOC_IA64_PCREL32MSB
: BFD_RELOC_IA64_PCREL32LSB
: BFD_RELOC_IA64_PCREL64MSB
: BFD_RELOC_IA64_PCREL64LSB
: BFD_RELOC_IA64_LTOFF_FPTR22
: BFD_RELOC_IA64_LTOFF_FPTR64I
: BFD_RELOC_IA64_LTOFF_FPTR32MSB
: BFD_RELOC_IA64_LTOFF_FPTR32LSB
: BFD_RELOC_IA64_LTOFF_FPTR64MSB
: BFD_RELOC_IA64_LTOFF_FPTR64LSB
: BFD_RELOC_IA64_SEGREL32MSB
: BFD_RELOC_IA64_SEGREL32LSB
: BFD_RELOC_IA64_SEGREL64MSB
: BFD_RELOC_IA64_SEGREL64LSB
: BFD_RELOC_IA64_SECREL32MSB
: BFD_RELOC_IA64_SECREL32LSB
: BFD_RELOC_IA64_SECREL64MSB
: BFD_RELOC_IA64_SECREL64LSB
: BFD_RELOC_IA64_REL32MSB
: BFD_RELOC_IA64_REL32LSB
: BFD_RELOC_IA64_REL64MSB
: BFD_RELOC_IA64_REL64LSB
: BFD_RELOC_IA64_LTV32MSB
: BFD_RELOC_IA64_LTV32LSB
: BFD_RELOC_IA64_LTV64MSB
: BFD_RELOC_IA64_LTV64LSB
: BFD_RELOC_IA64_IPLTMSB
: BFD_RELOC_IA64_IPLTLSB
: BFD_RELOC_IA64_COPY
: BFD_RELOC_IA64_LTOFF22X
: BFD_RELOC_IA64_LDXMOV
: BFD_RELOC_IA64_TPREL14
: BFD_RELOC_IA64_TPREL22
: BFD_RELOC_IA64_TPREL64I
: BFD_RELOC_IA64_TPREL64MSB
: BFD_RELOC_IA64_TPREL64LSB
: BFD_RELOC_IA64_LTOFF_TPREL22
: BFD_RELOC_IA64_DTPMOD64MSB
: BFD_RELOC_IA64_DTPMOD64LSB
: BFD_RELOC_IA64_LTOFF_DTPMOD22
: BFD_RELOC_IA64_DTPREL14
: BFD_RELOC_IA64_DTPREL22
: BFD_RELOC_IA64_DTPREL64I
: BFD_RELOC_IA64_DTPREL32MSB
: BFD_RELOC_IA64_DTPREL32LSB
: BFD_RELOC_IA64_DTPREL64MSB
: BFD_RELOC_IA64_DTPREL64LSB
: BFD_RELOC_IA64_LTOFF_DTPREL22

  Intel IA64 Relocations.

: BFD_RELOC_M68HC11_HI8

  Motorola 68HC11 reloc. This is the 8 bit high part of an absolute address.

: BFD_RELOC_M68HC11_LO8

  Motorola 68HC11 reloc. This is the 8 bit low part of an absolute address.

: BFD_RELOC_M68HC11_3B

  Motorola 68HC11 reloc. This is the 3 bit of a value.

: BFD_RELOC_M68HC11_RL_JUMP

  Motorola 68HC11 reloc. This reloc marks the beginning of a jump/call instruction. It is used for linker relaxation to correctly identify beginning of instruction and change some branches to use PC-relative addressing mode.

: BFD_RELOC_M68HC11_RL_GROUP

  Motorola 68HC11 reloc. This reloc marks a group of several instructions that gcc generates and for which the linker relaxation pass can modify and/or remove some of them.

: BFD_RELOC_M68HC11_LO16

  Motorola 68HC11 reloc. This is the 16-bit lower part of an address. It is used for ’call’ instruction to specify the symbol address without any special transformation (due to memory bank window).

: BFD_RELOC_M68HC11_PAGE

  Motorola 68HC11 reloc. This is a 8-bit reloc that specifies the page number of an address. It is used by ’call’ instruction to specify the page number of the symbol.

: BFD_RELOC_M68HC11_24

  Motorola 68HC11 reloc. This is a 24-bit reloc that represents the address with a 16-bit value and a 8-bit page number. The symbol address is transformed to follow the 16K memory bank of 68HC12 (seen as mapped in the window).

: BFD_RELOC_M68HC12_5B

  Motorola 68HC12 reloc. This is the 5 bits of a value.

: BFD_RELOC_XGATE_RL_JUMP

  Freescale XGATE reloc. This reloc marks the beginning of a bra/jal instruction.

: BFD_RELOC_XGATE_RL_GROUP

  Freescale XGATE reloc. This reloc marks a group of several instructions that gcc generates and for which the linker relaxation pass can modify and/or remove some of them.

: BFD_RELOC_XGATE_LO16

  Freescale XGATE reloc. This is the 16-bit lower part of an address. It is used for the ’16-bit’ instructions.

: BFD_RELOC_XGATE_GPAGE

  Freescale XGATE reloc.

: BFD_RELOC_XGATE_24

  Freescale XGATE reloc.

: BFD_RELOC_XGATE_PCREL_9

  Freescale XGATE reloc. This is a 9-bit pc-relative reloc.

: BFD_RELOC_XGATE_PCREL_10

  Freescale XGATE reloc. This is a 10-bit pc-relative reloc.

: BFD_RELOC_XGATE_IMM8_LO

  Freescale XGATE reloc. This is the 16-bit lower part of an address. It is used for the ’16-bit’ instructions.

: BFD_RELOC_XGATE_IMM8_HI

  Freescale XGATE reloc. This is the 16-bit higher part of an address. It is used for the ’16-bit’ instructions.

: BFD_RELOC_XGATE_IMM3

  Freescale XGATE reloc. This is a 3-bit pc-relative reloc.

: BFD_RELOC_XGATE_IMM4

  Freescale XGATE reloc. This is a 4-bit pc-relative reloc.

: BFD_RELOC_XGATE_IMM5

  Freescale XGATE reloc. This is a 5-bit pc-relative reloc.

: BFD_RELOC_M68HC12_9B

  Motorola 68HC12 reloc. This is the 9 bits of a value.

: BFD_RELOC_M68HC12_16B

  Motorola 68HC12 reloc. This is the 16 bits of a value.

: BFD_RELOC_M68HC12_9_PCREL

  Motorola 68HC12/XGATE reloc. This is a PCREL9 branch.

: BFD_RELOC_M68HC12_10_PCREL

  Motorola 68HC12/XGATE reloc. This is a PCREL10 branch.

: BFD_RELOC_M68HC12_LO8XG

  Motorola 68HC12/XGATE reloc. This is the 8 bit low part of an absolute address and immediately precedes a matching HI8XG part.

: BFD_RELOC_M68HC12_HI8XG

  Motorola 68HC12/XGATE reloc. This is the 8 bit high part of an absolute address and immediately follows a matching LO8XG part.

: BFD_RELOC_16C_NUM08
: BFD_RELOC_16C_NUM08_C
: BFD_RELOC_16C_NUM16
: BFD_RELOC_16C_NUM16_C
: BFD_RELOC_16C_NUM32
: BFD_RELOC_16C_NUM32_C
: BFD_RELOC_16C_DISP04
: BFD_RELOC_16C_DISP04_C
: BFD_RELOC_16C_DISP08
: BFD_RELOC_16C_DISP08_C
: BFD_RELOC_16C_DISP16
: BFD_RELOC_16C_DISP16_C
: BFD_RELOC_16C_DISP24
: BFD_RELOC_16C_DISP24_C
: BFD_RELOC_16C_DISP24a
: BFD_RELOC_16C_DISP24a_C
: BFD_RELOC_16C_REG04
: BFD_RELOC_16C_REG04_C
: BFD_RELOC_16C_REG04a
: BFD_RELOC_16C_REG04a_C
: BFD_RELOC_16C_REG14
: BFD_RELOC_16C_REG14_C
: BFD_RELOC_16C_REG16
: BFD_RELOC_16C_REG16_C
: BFD_RELOC_16C_REG20
: BFD_RELOC_16C_REG20_C
: BFD_RELOC_16C_ABS20
: BFD_RELOC_16C_ABS20_C
: BFD_RELOC_16C_ABS24
: BFD_RELOC_16C_ABS24_C
: BFD_RELOC_16C_IMM04
: BFD_RELOC_16C_IMM04_C
: BFD_RELOC_16C_IMM16
: BFD_RELOC_16C_IMM16_C
: BFD_RELOC_16C_IMM20
: BFD_RELOC_16C_IMM20_C
: BFD_RELOC_16C_IMM24
: BFD_RELOC_16C_IMM24_C
: BFD_RELOC_16C_IMM32
: BFD_RELOC_16C_IMM32_C

  NS CR16C Relocations.

: BFD_RELOC_CR16_NUM8
: BFD_RELOC_CR16_NUM16
: BFD_RELOC_CR16_NUM32
: BFD_RELOC_CR16_NUM32a
: BFD_RELOC_CR16_REGREL0
: BFD_RELOC_CR16_REGREL4
: BFD_RELOC_CR16_REGREL4a
: BFD_RELOC_CR16_REGREL14
: BFD_RELOC_CR16_REGREL14a
: BFD_RELOC_CR16_REGREL16
: BFD_RELOC_CR16_REGREL20
: BFD_RELOC_CR16_REGREL20a
: BFD_RELOC_CR16_ABS20
: BFD_RELOC_CR16_ABS24
: BFD_RELOC_CR16_IMM4
: BFD_RELOC_CR16_IMM8
: BFD_RELOC_CR16_IMM16
: BFD_RELOC_CR16_IMM20
: BFD_RELOC_CR16_IMM24
: BFD_RELOC_CR16_IMM32
: BFD_RELOC_CR16_IMM32a
: BFD_RELOC_CR16_DISP4
: BFD_RELOC_CR16_DISP8
: BFD_RELOC_CR16_DISP16
: BFD_RELOC_CR16_DISP20
: BFD_RELOC_CR16_DISP24
: BFD_RELOC_CR16_DISP24a
: BFD_RELOC_CR16_SWITCH8
: BFD_RELOC_CR16_SWITCH16
: BFD_RELOC_CR16_SWITCH32
: BFD_RELOC_CR16_GOT_REGREL20
: BFD_RELOC_CR16_GOTC_REGREL20
: BFD_RELOC_CR16_GLOB_DAT

  NS CR16 Relocations.

: BFD_RELOC_CRX_REL4
: BFD_RELOC_CRX_REL8
: BFD_RELOC_CRX_REL8_CMP
: BFD_RELOC_CRX_REL16
: BFD_RELOC_CRX_REL24
: BFD_RELOC_CRX_REL32
: BFD_RELOC_CRX_REGREL12
: BFD_RELOC_CRX_REGREL22
: BFD_RELOC_CRX_REGREL28
: BFD_RELOC_CRX_REGREL32
: BFD_RELOC_CRX_ABS16
: BFD_RELOC_CRX_ABS32
: BFD_RELOC_CRX_NUM8
: BFD_RELOC_CRX_NUM16
: BFD_RELOC_CRX_NUM32
: BFD_RELOC_CRX_IMM16
: BFD_RELOC_CRX_IMM32
: BFD_RELOC_CRX_SWITCH8
: BFD_RELOC_CRX_SWITCH16
: BFD_RELOC_CRX_SWITCH32

  NS CRX Relocations.

: BFD_RELOC_CRIS_BDISP8
: BFD_RELOC_CRIS_UNSIGNED_5
: BFD_RELOC_CRIS_SIGNED_6
: BFD_RELOC_CRIS_UNSIGNED_6
: BFD_RELOC_CRIS_SIGNED_8
: BFD_RELOC_CRIS_UNSIGNED_8
: BFD_RELOC_CRIS_SIGNED_16
: BFD_RELOC_CRIS_UNSIGNED_16
: BFD_RELOC_CRIS_LAPCQ_OFFSET
: BFD_RELOC_CRIS_UNSIGNED_4

  These relocs are only used within the CRIS assembler. They are not (at present) written to any object files.

: BFD_RELOC_CRIS_COPY
: BFD_RELOC_CRIS_GLOB_DAT
: BFD_RELOC_CRIS_JUMP_SLOT
: BFD_RELOC_CRIS_RELATIVE

  Relocs used in ELF shared libraries for CRIS.

: BFD_RELOC_CRIS_32_GOT

  32-bit offset to symbol-entry within GOT.

: BFD_RELOC_CRIS_16_GOT

  16-bit offset to symbol-entry within GOT.

: BFD_RELOC_CRIS_32_GOTPLT

  32-bit offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_CRIS_16_GOTPLT

  16-bit offset to symbol-entry within GOT, with PLT handling.

: BFD_RELOC_CRIS_32_GOTREL

  32-bit offset to symbol, relative to GOT.

: BFD_RELOC_CRIS_32_PLT_GOTREL

  32-bit offset to symbol with PLT entry, relative to GOT.

: BFD_RELOC_CRIS_32_PLT_PCREL

  32-bit offset to symbol with PLT entry, relative to this relocation.

: BFD_RELOC_CRIS_32_GOT_GD
: BFD_RELOC_CRIS_16_GOT_GD
: BFD_RELOC_CRIS_32_GD
: BFD_RELOC_CRIS_DTP
: BFD_RELOC_CRIS_32_DTPREL
: BFD_RELOC_CRIS_16_DTPREL
: BFD_RELOC_CRIS_32_GOT_TPREL
: BFD_RELOC_CRIS_16_GOT_TPREL
: BFD_RELOC_CRIS_32_TPREL
: BFD_RELOC_CRIS_16_TPREL
: BFD_RELOC_CRIS_DTPMOD
: BFD_RELOC_CRIS_32_IE

  Relocs used in TLS code for CRIS.

: BFD_RELOC_860_COPY
: BFD_RELOC_860_GLOB_DAT
: BFD_RELOC_860_JUMP_SLOT
: BFD_RELOC_860_RELATIVE
: BFD_RELOC_860_PC26
: BFD_RELOC_860_PLT26
: BFD_RELOC_860_PC16
: BFD_RELOC_860_LOW0
: BFD_RELOC_860_SPLIT0
: BFD_RELOC_860_LOW1
: BFD_RELOC_860_SPLIT1
: BFD_RELOC_860_LOW2
: BFD_RELOC_860_SPLIT2
: BFD_RELOC_860_LOW3
: BFD_RELOC_860_LOGOT0
: BFD_RELOC_860_SPGOT0
: BFD_RELOC_860_LOGOT1
: BFD_RELOC_860_SPGOT1
: BFD_RELOC_860_LOGOTOFF0
: BFD_RELOC_860_SPGOTOFF0
: BFD_RELOC_860_LOGOTOFF1
: BFD_RELOC_860_SPGOTOFF1
: BFD_RELOC_860_LOGOTOFF2
: BFD_RELOC_860_LOGOTOFF3
: BFD_RELOC_860_LOPC
: BFD_RELOC_860_HIGHADJ
: BFD_RELOC_860_HAGOT
: BFD_RELOC_860_HAGOTOFF
: BFD_RELOC_860_HAPC
: BFD_RELOC_860_HIGH
: BFD_RELOC_860_HIGOT
: BFD_RELOC_860_HIGOTOFF

  Intel i860 Relocations.

: BFD_RELOC_OR1K_REL_26
: BFD_RELOC_OR1K_GOTPC_HI16
: BFD_RELOC_OR1K_GOTPC_LO16
: BFD_RELOC_OR1K_GOT16
: BFD_RELOC_OR1K_PLT26
: BFD_RELOC_OR1K_GOTOFF_HI16
: BFD_RELOC_OR1K_GOTOFF_LO16
: BFD_RELOC_OR1K_COPY
: BFD_RELOC_OR1K_GLOB_DAT
: BFD_RELOC_OR1K_JMP_SLOT
: BFD_RELOC_OR1K_RELATIVE
: BFD_RELOC_OR1K_TLS_GD_HI16
: BFD_RELOC_OR1K_TLS_GD_LO16
: BFD_RELOC_OR1K_TLS_LDM_HI16
: BFD_RELOC_OR1K_TLS_LDM_LO16
: BFD_RELOC_OR1K_TLS_LDO_HI16
: BFD_RELOC_OR1K_TLS_LDO_LO16
: BFD_RELOC_OR1K_TLS_IE_HI16
: BFD_RELOC_OR1K_TLS_IE_LO16
: BFD_RELOC_OR1K_TLS_LE_HI16
: BFD_RELOC_OR1K_TLS_LE_LO16
: BFD_RELOC_OR1K_TLS_TPOFF
: BFD_RELOC_OR1K_TLS_DTPOFF
: BFD_RELOC_OR1K_TLS_DTPMOD

  OpenRISC 1000 Relocations.

: BFD_RELOC_H8_DIR16A8
: BFD_RELOC_H8_DIR16R8
: BFD_RELOC_H8_DIR24A8
: BFD_RELOC_H8_DIR24R8
: BFD_RELOC_H8_DIR32A16
: BFD_RELOC_H8_DISP32A16

  H8 elf Relocations.

: BFD_RELOC_XSTORMY16_REL_12
: BFD_RELOC_XSTORMY16_12
: BFD_RELOC_XSTORMY16_24
: BFD_RELOC_XSTORMY16_FPTR16

  Sony Xstormy16 Relocations.

: BFD_RELOC_RELC

  Self-describing complex relocations.

: BFD_RELOC_XC16X_PAG
: BFD_RELOC_XC16X_POF
: BFD_RELOC_XC16X_SEG
: BFD_RELOC_XC16X_SOF

  Infineon Relocations.

: BFD_RELOC_VAX_GLOB_DAT
: BFD_RELOC_VAX_JMP_SLOT
: BFD_RELOC_VAX_RELATIVE

  Relocations used by VAX ELF.

: BFD_RELOC_MT_PC16

  Morpho MT - 16 bit immediate relocation.

: BFD_RELOC_MT_HI16

  Morpho MT - Hi 16 bits of an address.

: BFD_RELOC_MT_LO16

  Morpho MT - Low 16 bits of an address.

: BFD_RELOC_MT_GNU_VTINHERIT

  Morpho MT - Used to tell the linker which vtable entries are used.

: BFD_RELOC_MT_GNU_VTENTRY

  Morpho MT - Used to tell the linker which vtable entries are used.

: BFD_RELOC_MT_PCINSN8

  Morpho MT - 8 bit immediate relocation.

: BFD_RELOC_MSP430_10_PCREL
: BFD_RELOC_MSP430_16_PCREL
: BFD_RELOC_MSP430_16
: BFD_RELOC_MSP430_16_PCREL_BYTE
: BFD_RELOC_MSP430_16_BYTE
: BFD_RELOC_MSP430_2X_PCREL
: BFD_RELOC_MSP430_RL_PCREL
: BFD_RELOC_MSP430_ABS8
: BFD_RELOC_MSP430X_PCR20_EXT_SRC
: BFD_RELOC_MSP430X_PCR20_EXT_DST
: BFD_RELOC_MSP430X_PCR20_EXT_ODST
: BFD_RELOC_MSP430X_ABS20_EXT_SRC
: BFD_RELOC_MSP430X_ABS20_EXT_DST
: BFD_RELOC_MSP430X_ABS20_EXT_ODST
: BFD_RELOC_MSP430X_ABS20_ADR_SRC
: BFD_RELOC_MSP430X_ABS20_ADR_DST
: BFD_RELOC_MSP430X_PCR16
: BFD_RELOC_MSP430X_PCR20_CALL
: BFD_RELOC_MSP430X_ABS16
: BFD_RELOC_MSP430_ABS_HI16
: BFD_RELOC_MSP430_PREL31
: BFD_RELOC_MSP430_SYM_DIFF

  msp430 specific relocation codes

: BFD_RELOC_NIOS2_S16
: BFD_RELOC_NIOS2_U16
: BFD_RELOC_NIOS2_CALL26
: BFD_RELOC_NIOS2_IMM5
: BFD_RELOC_NIOS2_CACHE_OPX
: BFD_RELOC_NIOS2_IMM6
: BFD_RELOC_NIOS2_IMM8
: BFD_RELOC_NIOS2_HI16
: BFD_RELOC_NIOS2_LO16
: BFD_RELOC_NIOS2_HIADJ16
: BFD_RELOC_NIOS2_GPREL
: BFD_RELOC_NIOS2_UJMP
: BFD_RELOC_NIOS2_CJMP
: BFD_RELOC_NIOS2_CALLR
: BFD_RELOC_NIOS2_ALIGN
: BFD_RELOC_NIOS2_GOT16
: BFD_RELOC_NIOS2_CALL16
: BFD_RELOC_NIOS2_GOTOFF_LO
: BFD_RELOC_NIOS2_GOTOFF_HA
: BFD_RELOC_NIOS2_PCREL_LO
: BFD_RELOC_NIOS2_PCREL_HA
: BFD_RELOC_NIOS2_TLS_GD16
: BFD_RELOC_NIOS2_TLS_LDM16
: BFD_RELOC_NIOS2_TLS_LDO16
: BFD_RELOC_NIOS2_TLS_IE16
: BFD_RELOC_NIOS2_TLS_LE16
: BFD_RELOC_NIOS2_TLS_DTPMOD
: BFD_RELOC_NIOS2_TLS_DTPREL
: BFD_RELOC_NIOS2_TLS_TPREL
: BFD_RELOC_NIOS2_COPY
: BFD_RELOC_NIOS2_GLOB_DAT
: BFD_RELOC_NIOS2_JUMP_SLOT
: BFD_RELOC_NIOS2_RELATIVE
: BFD_RELOC_NIOS2_GOTOFF
: BFD_RELOC_NIOS2_CALL26_NOAT
: BFD_RELOC_NIOS2_GOT_LO
: BFD_RELOC_NIOS2_GOT_HA
: BFD_RELOC_NIOS2_CALL_LO
: BFD_RELOC_NIOS2_CALL_HA
: BFD_RELOC_NIOS2_R2_S12
: BFD_RELOC_NIOS2_R2_I10_1_PCREL
: BFD_RELOC_NIOS2_R2_T1I7_1_PCREL
: BFD_RELOC_NIOS2_R2_T1I7_2
: BFD_RELOC_NIOS2_R2_T2I4
: BFD_RELOC_NIOS2_R2_T2I4_1
: BFD_RELOC_NIOS2_R2_T2I4_2
: BFD_RELOC_NIOS2_R2_X1I7_2
: BFD_RELOC_NIOS2_R2_X2L5
: BFD_RELOC_NIOS2_R2_F1I5_2
: BFD_RELOC_NIOS2_R2_L5I4X1
: BFD_RELOC_NIOS2_R2_T1X1I6
: BFD_RELOC_NIOS2_R2_T1X1I6_2

  Relocations used by the Altera Nios II core.

: BFD_RELOC_PRU_U16

  PRU LDI 16-bit unsigned data-memory relocation.

: BFD_RELOC_PRU_U16_PMEMIMM

  PRU LDI 16-bit unsigned instruction-memory relocation.

: BFD_RELOC_PRU_LDI32

  PRU relocation for two consecutive LDI load instructions that load a 32 bit value into a register. If the higher bits are all zero, then the second instruction may be relaxed.

: BFD_RELOC_PRU_S10_PCREL

  PRU QBBx 10-bit signed PC-relative relocation.

: BFD_RELOC_PRU_U8_PCREL

  PRU 8-bit unsigned relocation used for the LOOP instruction.

: BFD_RELOC_PRU_32_PMEM
: BFD_RELOC_PRU_16_PMEM

  PRU Program Memory relocations. Used to convert from byte addressing to 32-bit word addressing.

: BFD_RELOC_PRU_GNU_DIFF8
: BFD_RELOC_PRU_GNU_DIFF16
: BFD_RELOC_PRU_GNU_DIFF32
: BFD_RELOC_PRU_GNU_DIFF16_PMEM
: BFD_RELOC_PRU_GNU_DIFF32_PMEM

  PRU relocations to mark the difference of two local symbols. These are only needed to support linker relaxation and can be ignored when not relaxing. The field is set to the value of the difference assuming no relaxation. The relocation encodes the position of the second symbol so the linker can determine whether to adjust the field value. The PMEM variants encode the word difference, instead of byte difference between symbols.

: BFD_RELOC_IQ2000_OFFSET_16
: BFD_RELOC_IQ2000_OFFSET_21
: BFD_RELOC_IQ2000_UHI16

  IQ2000 Relocations.

: BFD_RELOC_XTENSA_RTLD

  Special Xtensa relocation used only by PLT entries in ELF shared objects to indicate that the runtime linker should set the value to one of its own internal functions or data structures.

: BFD_RELOC_XTENSA_GLOB_DAT
: BFD_RELOC_XTENSA_JMP_SLOT
: BFD_RELOC_XTENSA_RELATIVE

  Xtensa relocations for ELF shared objects.

: BFD_RELOC_XTENSA_PLT

  Xtensa relocation used in ELF object files for symbols that may require PLT entries. Otherwise, this is just a generic 32-bit relocation.

: BFD_RELOC_XTENSA_DIFF8
: BFD_RELOC_XTENSA_DIFF16
: BFD_RELOC_XTENSA_DIFF32

  Xtensa relocations to mark the difference of two local symbols. These are only needed to support linker relaxation and can be ignored when not relaxing. The field is set to the value of the difference assuming no relaxation. The relocation encodes the position of the first symbol so the linker can determine whether to adjust the field value.

: BFD_RELOC_XTENSA_SLOT0_OP
: BFD_RELOC_XTENSA_SLOT1_OP
: BFD_RELOC_XTENSA_SLOT2_OP
: BFD_RELOC_XTENSA_SLOT3_OP
: BFD_RELOC_XTENSA_SLOT4_OP
: BFD_RELOC_XTENSA_SLOT5_OP
: BFD_RELOC_XTENSA_SLOT6_OP
: BFD_RELOC_XTENSA_SLOT7_OP
: BFD_RELOC_XTENSA_SLOT8_OP
: BFD_RELOC_XTENSA_SLOT9_OP
: BFD_RELOC_XTENSA_SLOT10_OP
: BFD_RELOC_XTENSA_SLOT11_OP
: BFD_RELOC_XTENSA_SLOT12_OP
: BFD_RELOC_XTENSA_SLOT13_OP
: BFD_RELOC_XTENSA_SLOT14_OP

  Generic Xtensa relocations for instruction operands. Only the slot number is encoded in the relocation. The relocation applies to the last PC-relative immediate operand, or if there are no PC-relative immediates, to the last immediate operand.

: BFD_RELOC_XTENSA_SLOT0_ALT
: BFD_RELOC_XTENSA_SLOT1_ALT
: BFD_RELOC_XTENSA_SLOT2_ALT
: BFD_RELOC_XTENSA_SLOT3_ALT
: BFD_RELOC_XTENSA_SLOT4_ALT
: BFD_RELOC_XTENSA_SLOT5_ALT
: BFD_RELOC_XTENSA_SLOT6_ALT
: BFD_RELOC_XTENSA_SLOT7_ALT
: BFD_RELOC_XTENSA_SLOT8_ALT
: BFD_RELOC_XTENSA_SLOT9_ALT
: BFD_RELOC_XTENSA_SLOT10_ALT
: BFD_RELOC_XTENSA_SLOT11_ALT
: BFD_RELOC_XTENSA_SLOT12_ALT
: BFD_RELOC_XTENSA_SLOT13_ALT
: BFD_RELOC_XTENSA_SLOT14_ALT

  Alternate Xtensa relocations. Only the slot is encoded in the relocation. The meaning of these relocations is opcode-specific.

: BFD_RELOC_XTENSA_OP0
: BFD_RELOC_XTENSA_OP1
: BFD_RELOC_XTENSA_OP2

  Xtensa relocations for backward compatibility. These have all been replaced by BFD_RELOC_XTENSA_SLOT0_OP.

: BFD_RELOC_XTENSA_ASM_EXPAND

  Xtensa relocation to mark that the assembler expanded the instructions from an original target. The expansion size is encoded in the reloc size.

: BFD_RELOC_XTENSA_ASM_SIMPLIFY

  Xtensa relocation to mark that the linker should simplify assembler-expanded instructions. This is commonly used internally by the linker after analysis of a BFD_RELOC_XTENSA_ASM_EXPAND.

: BFD_RELOC_XTENSA_TLSDESC_FN
: BFD_RELOC_XTENSA_TLSDESC_ARG
: BFD_RELOC_XTENSA_TLS_DTPOFF
: BFD_RELOC_XTENSA_TLS_TPOFF
: BFD_RELOC_XTENSA_TLS_FUNC
: BFD_RELOC_XTENSA_TLS_ARG
: BFD_RELOC_XTENSA_TLS_CALL

  Xtensa TLS relocations.

: BFD_RELOC_Z80_DISP8

  8 bit signed offset in (ix+d) or (iy+d).

: BFD_RELOC_Z8K_DISP7

  DJNZ offset.

: BFD_RELOC_Z8K_CALLR

  CALR offset.

: BFD_RELOC_Z8K_IMM4L

  4 bit value.

: BFD_RELOC_LM32_CALL
: BFD_RELOC_LM32_BRANCH
: BFD_RELOC_LM32_16_GOT
: BFD_RELOC_LM32_GOTOFF_HI16
: BFD_RELOC_LM32_GOTOFF_LO16
: BFD_RELOC_LM32_COPY
: BFD_RELOC_LM32_GLOB_DAT
: BFD_RELOC_LM32_JMP_SLOT
: BFD_RELOC_LM32_RELATIVE

  Lattice Mico32 relocations.

: BFD_RELOC_MACH_O_SECTDIFF

  Difference between two section addreses. Must be followed by a BFD_RELOC_MACH_O_PAIR.

: BFD_RELOC_MACH_O_LOCAL_SECTDIFF

  Like BFD_RELOC_MACH_O_SECTDIFF but with a local symbol.

: BFD_RELOC_MACH_O_PAIR

  Pair of relocation. Contains the first symbol.

: BFD_RELOC_MACH_O_SUBTRACTOR32

  Symbol will be substracted. Must be followed by a BFD_RELOC_32.

: BFD_RELOC_MACH_O_SUBTRACTOR64

  Symbol will be substracted. Must be followed by a BFD_RELOC_64.

: BFD_RELOC_MACH_O_X86_64_BRANCH32
: BFD_RELOC_MACH_O_X86_64_BRANCH8

  PCREL relocations. They are marked as branch to create PLT entry if required.

: BFD_RELOC_MACH_O_X86_64_GOT

  Used when referencing a GOT entry.

: BFD_RELOC_MACH_O_X86_64_GOT_LOAD

  Used when loading a GOT entry with movq. It is specially marked so that the linker could optimize the movq to a leaq if possible.

: BFD_RELOC_MACH_O_X86_64_PCREL32_1

  Same as BFD_RELOC_32_PCREL but with an implicit -1 addend.

: BFD_RELOC_MACH_O_X86_64_PCREL32_2

  Same as BFD_RELOC_32_PCREL but with an implicit -2 addend.

: BFD_RELOC_MACH_O_X86_64_PCREL32_4

  Same as BFD_RELOC_32_PCREL but with an implicit -4 addend.

: BFD_RELOC_MACH_O_ARM64_ADDEND

  Addend for PAGE or PAGEOFF.

: BFD_RELOC_MACH_O_ARM64_GOT_LOAD_PAGE21

  Relative offset to page of GOT slot.

: BFD_RELOC_MACH_O_ARM64_GOT_LOAD_PAGEOFF12

  Relative offset within page of GOT slot.

: BFD_RELOC_MACH_O_ARM64_POINTER_TO_GOT

  Address of a GOT entry.

: BFD_RELOC_MICROBLAZE_32_LO

  This is a 32 bit reloc for the microblaze that stores the low 16 bits of a value

: BFD_RELOC_MICROBLAZE_32_LO_PCREL

  This is a 32 bit pc-relative reloc for the microblaze that stores the low 16 bits of a value

: BFD_RELOC_MICROBLAZE_32_ROSDA

  This is a 32 bit reloc for the microblaze that stores a value relative to the read-only small data area anchor

: BFD_RELOC_MICROBLAZE_32_RWSDA

  This is a 32 bit reloc for the microblaze that stores a value relative to the read-write small data area anchor

: BFD_RELOC_MICROBLAZE_32_SYM_OP_SYM

  This is a 32 bit reloc for the microblaze to handle expressions of the form "Symbol Op Symbol"

: BFD_RELOC_MICROBLAZE_64_NONE

  This is a 64 bit reloc that stores the 32 bit pc relative value in two words (with an imm instruction). No relocation is done here - only used for relaxing

: BFD_RELOC_MICROBLAZE_64_GOTPC

  This is a 64 bit reloc that stores the 32 bit pc relative value in two words (with an imm instruction). The relocation is PC-relative GOT offset

: BFD_RELOC_MICROBLAZE_64_GOT

  This is a 64 bit reloc that stores the 32 bit pc relative value in two words (with an imm instruction). The relocation is GOT offset

: BFD_RELOC_MICROBLAZE_64_PLT

  This is a 64 bit reloc that stores the 32 bit pc relative value in two words (with an imm instruction). The relocation is PC-relative offset into PLT

: BFD_RELOC_MICROBLAZE_64_GOTOFF

  This is a 64 bit reloc that stores the 32 bit GOT relative value in two words (with an imm instruction). The relocation is relative offset from _GLOBAL_OFFSET_TABLE_

: BFD_RELOC_MICROBLAZE_32_GOTOFF

  This is a 32 bit reloc that stores the 32 bit GOT relative value in a word. The relocation is relative offset from

: BFD_RELOC_MICROBLAZE_COPY

  This is used to tell the dynamic linker to copy the value out of the dynamic object into the runtime process image.

: BFD_RELOC_MICROBLAZE_64_TLS

  Unused Reloc

: BFD_RELOC_MICROBLAZE_64_TLSGD

  This is a 64 bit reloc that stores the 32 bit GOT relative value of the GOT TLS GD info entry in two words (with an imm instruction). The relocation is GOT offset.

: BFD_RELOC_MICROBLAZE_64_TLSLD

  This is a 64 bit reloc that stores the 32 bit GOT relative value of the GOT TLS LD info entry in two words (with an imm instruction). The relocation is GOT offset.

: BFD_RELOC_MICROBLAZE_32_TLSDTPMOD

  This is a 32 bit reloc that stores the Module ID to GOT(n).

: BFD_RELOC_MICROBLAZE_32_TLSDTPREL

  This is a 32 bit reloc that stores TLS offset to GOT(n+1).

: BFD_RELOC_MICROBLAZE_64_TLSDTPREL

  This is a 32 bit reloc for storing TLS offset to two words (uses imm instruction)

: BFD_RELOC_MICROBLAZE_64_TLSGOTTPREL

  This is a 64 bit reloc that stores 32-bit thread pointer relative offset to two words (uses imm instruction).

: BFD_RELOC_MICROBLAZE_64_TLSTPREL

  This is a 64 bit reloc that stores 32-bit thread pointer relative offset to two words (uses imm instruction).

: BFD_RELOC_AARCH64_RELOC_START

  AArch64 pseudo relocation code to mark the start of the AArch64 relocation enumerators. N.B. the order of the enumerators is important as several tables in the AArch64 bfd backend are indexed by these enumerators; make sure they are all synced.

: BFD_RELOC_AARCH64_NULL

  Deprecated AArch64 null relocation code.

: BFD_RELOC_AARCH64_NONE

  AArch64 null relocation code.

: BFD_RELOC_AARCH64_64
: BFD_RELOC_AARCH64_32
: BFD_RELOC_AARCH64_16

  Basic absolute relocations of N bits. These are equivalent to BFD_RELOC_N and they were added to assist the indexing of the howto table.

: BFD_RELOC_AARCH64_64_PCREL
: BFD_RELOC_AARCH64_32_PCREL
: BFD_RELOC_AARCH64_16_PCREL

  PC-relative relocations. These are equivalent to BFD_RELOC_N_PCREL and they were added to assist the indexing of the howto table.

: BFD_RELOC_AARCH64_MOVW_G0

  AArch64 MOV[NZK] instruction with most significant bits 0 to 15 of an unsigned address/value.

: BFD_RELOC_AARCH64_MOVW_G0_NC

  AArch64 MOV[NZK] instruction with less significant bits 0 to 15 of an address/value. No overflow checking.

: BFD_RELOC_AARCH64_MOVW_G1

  AArch64 MOV[NZK] instruction with most significant bits 16 to 31 of an unsigned address/value.

: BFD_RELOC_AARCH64_MOVW_G1_NC

  AArch64 MOV[NZK] instruction with less significant bits 16 to 31 of an address/value. No overflow checking.

: BFD_RELOC_AARCH64_MOVW_G2

  AArch64 MOV[NZK] instruction with most significant bits 32 to 47 of an unsigned address/value.

: BFD_RELOC_AARCH64_MOVW_G2_NC

  AArch64 MOV[NZK] instruction with less significant bits 32 to 47 of an address/value. No overflow checking.

: BFD_RELOC_AARCH64_MOVW_G3

  AArch64 MOV[NZK] instruction with most signficant bits 48 to 64 of a signed or unsigned address/value.

: BFD_RELOC_AARCH64_MOVW_G0_S

  AArch64 MOV[NZ] instruction with most significant bits 0 to 15 of a signed value. Changes instruction to MOVZ or MOVN depending on the value’s sign.

: BFD_RELOC_AARCH64_MOVW_G1_S

  AArch64 MOV[NZ] instruction with most significant bits 16 to 31 of a signed value. Changes instruction to MOVZ or MOVN depending on the value’s sign.

: BFD_RELOC_AARCH64_MOVW_G2_S

  AArch64 MOV[NZ] instruction with most significant bits 32 to 47 of a signed value. Changes instruction to MOVZ or MOVN depending on the value’s sign.

: BFD_RELOC_AARCH64_LD_LO19_PCREL

  AArch64 Load Literal instruction, holding a 19 bit pc-relative word offset. The lowest two bits must be zero and are not stored in the instruction, giving a 21 bit signed byte offset.

: BFD_RELOC_AARCH64_ADR_LO21_PCREL

  AArch64 ADR instruction, holding a simple 21 bit pc-relative byte offset.

: BFD_RELOC_AARCH64_ADR_HI21_PCREL

  AArch64 ADRP instruction, with bits 12 to 32 of a pc-relative page offset, giving a 4KB aligned page base address.

: BFD_RELOC_AARCH64_ADR_HI21_NC_PCREL

  AArch64 ADRP instruction, with bits 12 to 32 of a pc-relative page offset, giving a 4KB aligned page base address, but with no overflow checking.

: BFD_RELOC_AARCH64_ADD_LO12

  AArch64 ADD immediate instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_LDST8_LO12

  AArch64 8-bit load/store instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_TSTBR14

  AArch64 14 bit pc-relative test bit and branch. The lowest two bits must be zero and are not stored in the instruction, giving a 16 bit signed byte offset.

: BFD_RELOC_AARCH64_BRANCH19

  AArch64 19 bit pc-relative conditional branch and compare & branch. The lowest two bits must be zero and are not stored in the instruction, giving a 21 bit signed byte offset.

: BFD_RELOC_AARCH64_JUMP26

  AArch64 26 bit pc-relative unconditional branch. The lowest two bits must be zero and are not stored in the instruction, giving a 28 bit signed byte offset.

: BFD_RELOC_AARCH64_CALL26

  AArch64 26 bit pc-relative unconditional branch and link. The lowest two bits must be zero and are not stored in the instruction, giving a 28 bit signed byte offset.

: BFD_RELOC_AARCH64_LDST16_LO12

  AArch64 16-bit load/store instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_LDST32_LO12

  AArch64 32-bit load/store instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_LDST64_LO12

  AArch64 64-bit load/store instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_LDST128_LO12

  AArch64 128-bit load/store instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_GOT_LD_PREL19

  AArch64 Load Literal instruction, holding a 19 bit PC relative word offset of the global offset table entry for a symbol. The lowest two bits must be zero and are not stored in the instruction, giving a 21 bit signed byte offset. This relocation type requires signed overflow checking.

: BFD_RELOC_AARCH64_ADR_GOT_PAGE

  Get to the page base of the global offset table entry for a symbol as part of an ADRP instruction using a 21 bit PC relative value.Used in conjunction with BFD_RELOC_AARCH64_LD64_GOT_LO12_NC.

: BFD_RELOC_AARCH64_LD64_GOT_LO12_NC

  Unsigned 12 bit byte offset for 64 bit load/store from the page of the GOT entry for this symbol. Used in conjunction with BFD_RELOC_AARCH64_ADR_GOT_PAGE. Valid in LP64 ABI only.

: BFD_RELOC_AARCH64_LD32_GOT_LO12_NC

  Unsigned 12 bit byte offset for 32 bit load/store from the page of the GOT entry for this symbol. Used in conjunction with BFD_RELOC_AARCH64_ADR_GOT_PAGE. Valid in ILP32 ABI only.

: BFD_RELOC_AARCH64_MOVW_GOTOFF_G0_NC

  Unsigned 16 bit byte offset for 64 bit load/store from the GOT entry for this symbol. Valid in LP64 ABI only.

: BFD_RELOC_AARCH64_MOVW_GOTOFF_G1

  Unsigned 16 bit byte higher offset for 64 bit load/store from the GOT entry for this symbol. Valid in LP64 ABI only.

: BFD_RELOC_AARCH64_LD64_GOTOFF_LO15

  Unsigned 15 bit byte offset for 64 bit load/store from the page of the GOT entry for this symbol. Valid in LP64 ABI only.

: BFD_RELOC_AARCH64_LD32_GOTPAGE_LO14

  Scaled 14 bit byte offset to the page base of the global offset table.

: BFD_RELOC_AARCH64_LD64_GOTPAGE_LO15

  Scaled 15 bit byte offset to the page base of the global offset table.

: BFD_RELOC_AARCH64_TLSGD_ADR_PAGE21

  Get to the page base of the global offset table entry for a symbols tls_index structure as part of an adrp instruction using a 21 bit PC relative value. Used in conjunction with BFD_RELOC_AARCH64_TLSGD_ADD_LO12_NC.

: BFD_RELOC_AARCH64_TLSGD_ADR_PREL21

  AArch64 TLS General Dynamic

: BFD_RELOC_AARCH64_TLSGD_ADD_LO12_NC

  Unsigned 12 bit byte offset to global offset table entry for a symbols tls_index structure. Used in conjunction with BFD_RELOC_AARCH64_TLSGD_ADR_PAGE21.

: BFD_RELOC_AARCH64_TLSGD_MOVW_G0_NC

  AArch64 TLS General Dynamic relocation.

: BFD_RELOC_AARCH64_TLSGD_MOVW_G1

  AArch64 TLS General Dynamic relocation.

: BFD_RELOC_AARCH64_TLSIE_ADR_GOTTPREL_PAGE21

  AArch64 TLS INITIAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSIE_LD64_GOTTPREL_LO12_NC

  AArch64 TLS INITIAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSIE_LD32_GOTTPREL_LO12_NC

  AArch64 TLS INITIAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSIE_LD_GOTTPREL_PREL19

  AArch64 TLS INITIAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSIE_MOVW_GOTTPREL_G0_NC

  AArch64 TLS INITIAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSIE_MOVW_GOTTPREL_G1

  AArch64 TLS INITIAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLD_ADD_DTPREL_HI12

  bit[23:12] of byte offset to module TLS base address.

: BFD_RELOC_AARCH64_TLSLD_ADD_DTPREL_LO12

  Unsigned 12 bit byte offset to module TLS base address.

: BFD_RELOC_AARCH64_TLSLD_ADD_DTPREL_LO12_NC

  No overflow check version of BFD_RELOC_AARCH64_TLSLD_ADD_DTPREL_LO12.

: BFD_RELOC_AARCH64_TLSLD_ADD_LO12_NC

  Unsigned 12 bit byte offset to global offset table entry for a symbols tls_index structure. Used in conjunction with BFD_RELOC_AARCH64_TLSLD_ADR_PAGE21.

: BFD_RELOC_AARCH64_TLSLD_ADR_PAGE21

  GOT entry page address for AArch64 TLS Local Dynamic, used with ADRP instruction.

: BFD_RELOC_AARCH64_TLSLD_ADR_PREL21

  GOT entry address for AArch64 TLS Local Dynamic, used with ADR instruction.

: BFD_RELOC_AARCH64_TLSLD_LDST16_DTPREL_LO12

  bit[11:1] of byte offset to module TLS base address, encoded in ldst instructions.

: BFD_RELOC_AARCH64_TLSLD_LDST16_DTPREL_LO12_NC

  Similar as BFD_RELOC_AARCH64_TLSLD_LDST16_DTPREL_LO12, but no overflow check.

: BFD_RELOC_AARCH64_TLSLD_LDST32_DTPREL_LO12

  bit[11:2] of byte offset to module TLS base address, encoded in ldst instructions.

: BFD_RELOC_AARCH64_TLSLD_LDST32_DTPREL_LO12_NC

  Similar as BFD_RELOC_AARCH64_TLSLD_LDST32_DTPREL_LO12, but no overflow check.

: BFD_RELOC_AARCH64_TLSLD_LDST64_DTPREL_LO12

  bit[11:3] of byte offset to module TLS base address, encoded in ldst instructions.

: BFD_RELOC_AARCH64_TLSLD_LDST64_DTPREL_LO12_NC

  Similar as BFD_RELOC_AARCH64_TLSLD_LDST64_DTPREL_LO12, but no overflow check.

: BFD_RELOC_AARCH64_TLSLD_LDST8_DTPREL_LO12

  bit[11:0] of byte offset to module TLS base address, encoded in ldst instructions.

: BFD_RELOC_AARCH64_TLSLD_LDST8_DTPREL_LO12_NC

  Similar as BFD_RELOC_AARCH64_TLSLD_LDST8_DTPREL_LO12, but no overflow check.

: BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G0

  bit[15:0] of byte offset to module TLS base address.

: BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G0_NC

  No overflow check version of BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G0

: BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G1

  bit[31:16] of byte offset to module TLS base address.

: BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G1_NC

  No overflow check version of BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G1

: BFD_RELOC_AARCH64_TLSLD_MOVW_DTPREL_G2

  bit[47:32] of byte offset to module TLS base address.

: BFD_RELOC_AARCH64_TLSLE_MOVW_TPREL_G2

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_MOVW_TPREL_G1

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_MOVW_TPREL_G1_NC

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_MOVW_TPREL_G0

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_MOVW_TPREL_G0_NC

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_ADD_TPREL_HI12

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_ADD_TPREL_LO12

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSLE_ADD_TPREL_LO12_NC

  AArch64 TLS LOCAL EXEC relocation.

: BFD_RELOC_AARCH64_TLSDESC_LD_PREL19

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_ADR_PREL21

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_ADR_PAGE21

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_LD64_LO12

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_LD32_LO12_NC

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_ADD_LO12

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_OFF_G1

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_OFF_G0_NC

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_LDR

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_ADD

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_TLSDESC_CALL

  AArch64 TLS DESC relocation.

: BFD_RELOC_AARCH64_COPY

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_GLOB_DAT

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_JUMP_SLOT

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_RELATIVE

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_TLS_DTPMOD

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_TLS_DTPREL

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_TLS_TPREL

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_TLSDESC

  AArch64 TLS relocation.

: BFD_RELOC_AARCH64_IRELATIVE

  AArch64 support for STT_GNU_IFUNC.

: BFD_RELOC_AARCH64_RELOC_END

  AArch64 pseudo relocation code to mark the end of the AArch64 relocation enumerators that have direct mapping to ELF reloc codes. There are a few more enumerators after this one; those are mainly used by the AArch64 assembler for the internal fixup or to select one of the above enumerators.

: BFD_RELOC_AARCH64_GAS_INTERNAL_FIXUP

  AArch64 pseudo relocation code to be used internally by the AArch64 assembler and not (currently) written to any object files.

: BFD_RELOC_AARCH64_LDST_LO12

  AArch64 unspecified load/store instruction, holding bits 0 to 11 of the address. Used in conjunction with BFD_RELOC_AARCH64_ADR_HI21_PCREL.

: BFD_RELOC_AARCH64_TLSLD_LDST_DTPREL_LO12

  AArch64 pseudo relocation code for TLS local dynamic mode. It’s to be used internally by the AArch64 assembler and not (currently) written to any object files.

: BFD_RELOC_AARCH64_TLSLD_LDST_DTPREL_LO12_NC

  Similar as BFD_RELOC_AARCH64_TLSLD_LDST_DTPREL_LO12, but no overflow check.

: BFD_RELOC_AARCH64_LD_GOT_LO12_NC

  AArch64 pseudo relocation code to be used internally by the AArch64 assembler and not (currently) written to any object files.

: BFD_RELOC_AARCH64_TLSIE_LD_GOTTPREL_LO12_NC

  AArch64 pseudo relocation code to be used internally by the AArch64 assembler and not (currently) written to any object files.

: BFD_RELOC_AARCH64_TLSDESC_LD_LO12_NC

  AArch64 pseudo relocation code to be used internally by the AArch64 assembler and not (currently) written to any object files.

: BFD_RELOC_TILEPRO_COPY
: BFD_RELOC_TILEPRO_GLOB_DAT
: BFD_RELOC_TILEPRO_JMP_SLOT
: BFD_RELOC_TILEPRO_RELATIVE
: BFD_RELOC_TILEPRO_BROFF_X1
: BFD_RELOC_TILEPRO_JOFFLONG_X1
: BFD_RELOC_TILEPRO_JOFFLONG_X1_PLT
: BFD_RELOC_TILEPRO_IMM8_X0
: BFD_RELOC_TILEPRO_IMM8_Y0
: BFD_RELOC_TILEPRO_IMM8_X1
: BFD_RELOC_TILEPRO_IMM8_Y1
: BFD_RELOC_TILEPRO_DEST_IMM8_X1
: BFD_RELOC_TILEPRO_MT_IMM15_X1
: BFD_RELOC_TILEPRO_MF_IMM15_X1
: BFD_RELOC_TILEPRO_IMM16_X0
: BFD_RELOC_TILEPRO_IMM16_X1
: BFD_RELOC_TILEPRO_IMM16_X0_LO
: BFD_RELOC_TILEPRO_IMM16_X1_LO
: BFD_RELOC_TILEPRO_IMM16_X0_HI
: BFD_RELOC_TILEPRO_IMM16_X1_HI
: BFD_RELOC_TILEPRO_IMM16_X0_HA
: BFD_RELOC_TILEPRO_IMM16_X1_HA
: BFD_RELOC_TILEPRO_IMM16_X0_PCREL
: BFD_RELOC_TILEPRO_IMM16_X1_PCREL
: BFD_RELOC_TILEPRO_IMM16_X0_LO_PCREL
: BFD_RELOC_TILEPRO_IMM16_X1_LO_PCREL
: BFD_RELOC_TILEPRO_IMM16_X0_HI_PCREL
: BFD_RELOC_TILEPRO_IMM16_X1_HI_PCREL
: BFD_RELOC_TILEPRO_IMM16_X0_HA_PCREL
: BFD_RELOC_TILEPRO_IMM16_X1_HA_PCREL
: BFD_RELOC_TILEPRO_IMM16_X0_GOT
: BFD_RELOC_TILEPRO_IMM16_X1_GOT
: BFD_RELOC_TILEPRO_IMM16_X0_GOT_LO
: BFD_RELOC_TILEPRO_IMM16_X1_GOT_LO
: BFD_RELOC_TILEPRO_IMM16_X0_GOT_HI
: BFD_RELOC_TILEPRO_IMM16_X1_GOT_HI
: BFD_RELOC_TILEPRO_IMM16_X0_GOT_HA
: BFD_RELOC_TILEPRO_IMM16_X1_GOT_HA
: BFD_RELOC_TILEPRO_MMSTART_X0
: BFD_RELOC_TILEPRO_MMEND_X0
: BFD_RELOC_TILEPRO_MMSTART_X1
: BFD_RELOC_TILEPRO_MMEND_X1
: BFD_RELOC_TILEPRO_SHAMT_X0
: BFD_RELOC_TILEPRO_SHAMT_X1
: BFD_RELOC_TILEPRO_SHAMT_Y0
: BFD_RELOC_TILEPRO_SHAMT_Y1
: BFD_RELOC_TILEPRO_TLS_GD_CALL
: BFD_RELOC_TILEPRO_IMM8_X0_TLS_GD_ADD
: BFD_RELOC_TILEPRO_IMM8_X1_TLS_GD_ADD
: BFD_RELOC_TILEPRO_IMM8_Y0_TLS_GD_ADD
: BFD_RELOC_TILEPRO_IMM8_Y1_TLS_GD_ADD
: BFD_RELOC_TILEPRO_TLS_IE_LOAD
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_GD
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_GD
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_GD_LO
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_GD_LO
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_GD_HI
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_GD_HI
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_GD_HA
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_GD_HA
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_IE
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_IE
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_IE_LO
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_IE_LO
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_IE_HI
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_IE_HI
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_IE_HA
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_IE_HA
: BFD_RELOC_TILEPRO_TLS_DTPMOD32
: BFD_RELOC_TILEPRO_TLS_DTPOFF32
: BFD_RELOC_TILEPRO_TLS_TPOFF32
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_LE
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_LE
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_LE_LO
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_LE_LO
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_LE_HI
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_LE_HI
: BFD_RELOC_TILEPRO_IMM16_X0_TLS_LE_HA
: BFD_RELOC_TILEPRO_IMM16_X1_TLS_LE_HA

  Tilera TILEPro Relocations.

: BFD_RELOC_TILEGX_HW0
: BFD_RELOC_TILEGX_HW1
: BFD_RELOC_TILEGX_HW2
: BFD_RELOC_TILEGX_HW3
: BFD_RELOC_TILEGX_HW0_LAST
: BFD_RELOC_TILEGX_HW1_LAST
: BFD_RELOC_TILEGX_HW2_LAST
: BFD_RELOC_TILEGX_COPY
: BFD_RELOC_TILEGX_GLOB_DAT
: BFD_RELOC_TILEGX_JMP_SLOT
: BFD_RELOC_TILEGX_RELATIVE
: BFD_RELOC_TILEGX_BROFF_X1
: BFD_RELOC_TILEGX_JUMPOFF_X1
: BFD_RELOC_TILEGX_JUMPOFF_X1_PLT
: BFD_RELOC_TILEGX_IMM8_X0
: BFD_RELOC_TILEGX_IMM8_Y0
: BFD_RELOC_TILEGX_IMM8_X1
: BFD_RELOC_TILEGX_IMM8_Y1
: BFD_RELOC_TILEGX_DEST_IMM8_X1
: BFD_RELOC_TILEGX_MT_IMM14_X1
: BFD_RELOC_TILEGX_MF_IMM14_X1
: BFD_RELOC_TILEGX_MMSTART_X0
: BFD_RELOC_TILEGX_MMEND_X0
: BFD_RELOC_TILEGX_SHAMT_X0
: BFD_RELOC_TILEGX_SHAMT_X1
: BFD_RELOC_TILEGX_SHAMT_Y0
: BFD_RELOC_TILEGX_SHAMT_Y1
: BFD_RELOC_TILEGX_IMM16_X0_HW0
: BFD_RELOC_TILEGX_IMM16_X1_HW0
: BFD_RELOC_TILEGX_IMM16_X0_HW1
: BFD_RELOC_TILEGX_IMM16_X1_HW1
: BFD_RELOC_TILEGX_IMM16_X0_HW2
: BFD_RELOC_TILEGX_IMM16_X1_HW2
: BFD_RELOC_TILEGX_IMM16_X0_HW3
: BFD_RELOC_TILEGX_IMM16_X1_HW3
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST
: BFD_RELOC_TILEGX_IMM16_X0_HW2_LAST
: BFD_RELOC_TILEGX_IMM16_X1_HW2_LAST
: BFD_RELOC_TILEGX_IMM16_X0_HW0_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW0_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW1_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW1_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW2_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW2_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW3_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW3_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW2_LAST_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW2_LAST_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW0_GOT
: BFD_RELOC_TILEGX_IMM16_X1_HW0_GOT
: BFD_RELOC_TILEGX_IMM16_X0_HW0_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW0_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW1_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW1_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW2_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW2_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST_GOT
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST_GOT
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST_GOT
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST_GOT
: BFD_RELOC_TILEGX_IMM16_X0_HW3_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW3_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW0_TLS_GD
: BFD_RELOC_TILEGX_IMM16_X1_HW0_TLS_GD
: BFD_RELOC_TILEGX_IMM16_X0_HW0_TLS_LE
: BFD_RELOC_TILEGX_IMM16_X1_HW0_TLS_LE
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST_TLS_LE
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST_TLS_LE
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST_TLS_LE
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST_TLS_LE
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST_TLS_GD
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST_TLS_GD
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST_TLS_GD
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST_TLS_GD
: BFD_RELOC_TILEGX_IMM16_X0_HW0_TLS_IE
: BFD_RELOC_TILEGX_IMM16_X1_HW0_TLS_IE
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW2_LAST_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X1_HW2_LAST_PLT_PCREL
: BFD_RELOC_TILEGX_IMM16_X0_HW0_LAST_TLS_IE
: BFD_RELOC_TILEGX_IMM16_X1_HW0_LAST_TLS_IE
: BFD_RELOC_TILEGX_IMM16_X0_HW1_LAST_TLS_IE
: BFD_RELOC_TILEGX_IMM16_X1_HW1_LAST_TLS_IE
: BFD_RELOC_TILEGX_TLS_DTPMOD64
: BFD_RELOC_TILEGX_TLS_DTPOFF64
: BFD_RELOC_TILEGX_TLS_TPOFF64
: BFD_RELOC_TILEGX_TLS_DTPMOD32
: BFD_RELOC_TILEGX_TLS_DTPOFF32
: BFD_RELOC_TILEGX_TLS_TPOFF32
: BFD_RELOC_TILEGX_TLS_GD_CALL
: BFD_RELOC_TILEGX_IMM8_X0_TLS_GD_ADD
: BFD_RELOC_TILEGX_IMM8_X1_TLS_GD_ADD
: BFD_RELOC_TILEGX_IMM8_Y0_TLS_GD_ADD
: BFD_RELOC_TILEGX_IMM8_Y1_TLS_GD_ADD
: BFD_RELOC_TILEGX_TLS_IE_LOAD
: BFD_RELOC_TILEGX_IMM8_X0_TLS_ADD
: BFD_RELOC_TILEGX_IMM8_X1_TLS_ADD
: BFD_RELOC_TILEGX_IMM8_Y0_TLS_ADD
: BFD_RELOC_TILEGX_IMM8_Y1_TLS_ADD

  Tilera TILE-Gx Relocations.

: BFD_RELOC_EPIPHANY_SIMM8

  Adapteva EPIPHANY - 8 bit signed pc-relative displacement

: BFD_RELOC_EPIPHANY_SIMM24

  Adapteva EPIPHANY - 24 bit signed pc-relative displacement

: BFD_RELOC_EPIPHANY_HIGH

  Adapteva EPIPHANY - 16 most-significant bits of absolute address

: BFD_RELOC_EPIPHANY_LOW

  Adapteva EPIPHANY - 16 least-significant bits of absolute address

: BFD_RELOC_EPIPHANY_SIMM11

  Adapteva EPIPHANY - 11 bit signed number - add/sub immediate

: BFD_RELOC_EPIPHANY_IMM11

  Adapteva EPIPHANY - 11 bit sign-magnitude number (ld/st displacement)

: BFD_RELOC_EPIPHANY_IMM8

  Adapteva EPIPHANY - 8 bit immediate for 16 bit mov instruction.

: BFD_RELOC_VISIUM_HI16
: BFD_RELOC_VISIUM_LO16
: BFD_RELOC_VISIUM_IM16
: BFD_RELOC_VISIUM_REL16
: BFD_RELOC_VISIUM_HI16_PCREL
: BFD_RELOC_VISIUM_LO16_PCREL
: BFD_RELOC_VISIUM_IM16_PCREL

  Visium Relocations.

: BFD_RELOC_WASM32_LEB128
: BFD_RELOC_WASM32_LEB128_GOT
: BFD_RELOC_WASM32_LEB128_GOT_CODE
: BFD_RELOC_WASM32_LEB128_PLT
: BFD_RELOC_WASM32_PLT_INDEX
: BFD_RELOC_WASM32_ABS32_CODE
: BFD_RELOC_WASM32_COPY
: BFD_RELOC_WASM32_CODE_POINTER
: BFD_RELOC_WASM32_INDEX
: BFD_RELOC_WASM32_PLT_SIG

  WebAssembly relocations.

    typedef enum bfd_reloc_code_real bfd_reloc_code_real_type;

#### 2.10.2.2 `bfd_reloc_type_lookup`

Synopsis

    reloc_howto_type *bfd_reloc_type_lookup
       (bfd *abfd, bfd_reloc_code_real_type code);
    reloc_howto_type *bfd_reloc_name_lookup
       (bfd *abfd, const char *reloc_name);

Description
Return a pointer to a howto structure which, when invoked, will perform the relocation code on data from the architecture noted.

#### 2.10.2.3 `bfd_default_reloc_type_lookup`

Synopsis

    reloc_howto_type *bfd_default_reloc_type_lookup
       (bfd *abfd, bfd_reloc_code_real_type  code);

Description
Provides a default relocation lookup routine for any architecture.

#### 2.10.2.4 `bfd_get_reloc_code_name`

Synopsis

    const char *bfd_get_reloc_code_name (bfd_reloc_code_real_type code);

Description
Provides a printable name for the supplied relocation code. Useful mainly for printing error messages.

#### 2.10.2.5 `bfd_generic_relax_section`

Synopsis

    bfd_boolean bfd_generic_relax_section
       (bfd *abfd,
        asection *section,
        struct bfd_link_info *,
        bfd_boolean *);

Description
Provides default handling for relaxing for back ends which don’t do relaxing.

#### 2.10.2.6 `bfd_generic_gc_sections`

Synopsis

    bfd_boolean bfd_generic_gc_sections
       (bfd *, struct bfd_link_info *);

Description
Provides default handling for relaxing for back ends which don’t do section gc – i.e., does nothing.

#### 2.10.2.7 `bfd_generic_lookup_section_flags`

Synopsis

    bfd_boolean bfd_generic_lookup_section_flags
       (struct bfd_link_info *, struct flag_info *, asection *);

Description
Provides default handling for section flags lookup – i.e., does nothing. Returns FALSE if the section should be omitted, otherwise TRUE.

#### 2.10.2.8 `bfd_generic_merge_sections`

Synopsis

    bfd_boolean bfd_generic_merge_sections
       (bfd *, struct bfd_link_info *);

Description
Provides default handling for SEC_MERGE section merging for back ends which don’t have SEC_MERGE support – i.e., does nothing.

#### 2.10.2.9 `bfd_generic_get_relocated_section_contents`

Synopsis

    bfd_byte *bfd_generic_get_relocated_section_contents
       (bfd *abfd,
        struct bfd_link_info *link_info,
        struct bfd_link_order *link_order,
        bfd_byte *data,
        bfd_boolean relocatable,
        asymbol **symbols);

Description
Provides default handling of relocation effort for back ends which can’t be bothered to do it efficiently.

#### 2.10.2.10 `_bfd_generic_set_reloc`

Synopsis

    void _bfd_generic_set_reloc
       (bfd *abfd,
        sec_ptr section,
        arelent **relptr,
        unsigned int count);

Description
Installs a new set of internal relocations in SECTION.

#### 2.10.2.11 `_bfd_unrecognized_reloc`

Synopsis

    bfd_boolean _bfd_unrecognized_reloc
       (bfd * abfd,
        sec_ptr section,
        unsigned int r_type);

Description
Reports an unrecognized reloc. Written as a function in order to reduce code duplication. Returns FALSE so that it can be called from a return statement.

Previous: typedef arelent, Up: Relocations [Contents][Index]