Next: SH Options, Previous: S/390 and zSeries Options, Up: Submodel Options [Contents][Index]

#### 3.18.42 Score Options

These options are defined for Score implementations:

`-meb`

  Compile code for big-endian mode. This is the default.

`-mel`

  Compile code for little-endian mode.

`-mnhwloop`

  Disable generation of `bcnz` instructions.

`-muls`

  Enable generation of unaligned load and store instructions.

`-mmac`

  Enable the use of multiply-accumulate instructions. Disabled by default.

`-mscore5`

  Specify the SCORE5 as the target architecture.

`-mscore5u`

  Specify the SCORE5U of the target architecture.

`-mscore7`

  Specify the SCORE7 as the target architecture. This is the default.

`-mscore7d`

  Specify the SCORE7D as the target architecture.