Next: i386 Features, Previous: ARC Features, Up: Standard Target Features [Contents][Index]

#### G.5.3 ARM Features

The ‘`org.gnu.gdb.arm.core`’ feature is required for non-M-profile ARM targets. It should contain registers ‘`r0`’ through ‘`r13`’, ‘`sp`’, ‘`lr`’, ‘`pc`’, and ‘`cpsr`’.

For M-profile targets (e.g. Cortex-M3), the ‘`org.gnu.gdb.arm.core`’ feature is replaced by ‘`org.gnu.gdb.arm.m-profile`’. It should contain registers ‘`r0`’ through ‘`r13`’, ‘`sp`’, ‘`lr`’, ‘`pc`’, and ‘`xpsr`’.

The ‘`org.gnu.gdb.arm.fpa`’ feature is optional. If present, it should contain registers ‘`f0`’ through ‘`f7`’ and ‘`fps`’.

The ‘`org.gnu.gdb.xscale.iwmmxt`’ feature is optional. If present, it should contain at least registers ‘`wR0`’ through ‘`wR15`’ and ‘`wCGR0`’ through ‘`wCGR3`’. The ‘`wCID`’, ‘`wCon`’, ‘`wCSSF`’, and ‘`wCASF`’ registers are optional.

The ‘`org.gnu.gdb.arm.vfp`’ feature is optional. If present, it should contain at least registers ‘`d0`’ through ‘`d15`’. If they are present, ‘`d16`’ through ‘`d31`’ should also be included. GDB will synthesize the single-precision registers from halves of the double-precision registers.

The ‘`org.gnu.gdb.arm.neon`’ feature is optional. It does not need to contain registers; it instructs GDB to display the VFP double-precision registers as vectors and to synthesize the quad-precision registers from pairs of double-precision registers. If this feature is present, ‘`org.gnu.gdb.arm.vfp`’ must also be present and include 32 double-precision registers.