Next: MSP430 Built-in Functions, Previous: MIPS SIMD Architecture (MSA) Support, Up: Target Builtins [Contents][Index]

#### 6.60.17 Other MIPS Built-in Functions

GCC provides other MIPS-specific built-in functions:

`void __builtin_mips_cache (int op, const volatile void *addr)`

  Insert a ‘`cache`’ instruction with operands op and addr. GCC defines the preprocessor macro `___GCC_HAVE_BUILTIN_MIPS_CACHE` when this function is available.

`unsigned int __builtin_mips_get_fcsr (void)`
`void __builtin_mips_set_fcsr (unsigned int value)`

  Get and set the contents of the floating-point control and status register (FPU control register 31). These functions are only available in hard-float code but can be called in both MIPS16 and non-MIPS16 contexts.

  `__builtin_mips_set_fcsr` can be used to change any bit of the register except the condition codes, which GCC assumes are preserved.