Next: SH64 Syntax, Up: SH64-Dependent [Contents][Index]

#### 9.43.1 Options

`-isa=sh4 | sh4a`

  Specify the sh4 or sh4a instruction set.

`-isa=dsp`

  Enable sh-dsp insns, and disable sh3e / sh4 insns.

`-isa=fp`

  Enable sh2e, sh3e, sh4, and sh4a insn sets.

`-isa=all`

  Enable sh1, sh2, sh2e, sh3, sh3e, sh4, sh4a, and sh-dsp insn sets.

`-isa=shmedia | -isa=shcompact`

  Specify the default instruction set. `SHmedia` specifies the 32-bit opcodes, and `SHcompact` specifies the 16-bit opcodes compatible with previous SH families. The default depends on the ABI selected; the default for the 64-bit ABI is SHmedia, and the default for the 32-bit ABI is SHcompact. If neither the ABI nor the ISA is specified, the default is 32-bit SHcompact.

  Note that the `.mode` pseudo-op is not permitted if the ISA is not specified on the command line.

`-abi=32 | -abi=64`

  Specify the default ABI. If the ISA is specified and the ABI is not, the default ABI depends on the ISA, with SHmedia defaulting to 64-bit and SHcompact defaulting to 32-bit.

  Note that the `.abi` pseudo-op is not permitted if the ABI is not specified on the command line. When the ABI is specified on the command line, any `.abi` pseudo-ops in the source must match it.

`-shcompact-const-crange`

  Emit code-range descriptors for constants in SHcompact code sections.

`-no-mix`

  Disallow SHmedia code in the same section as constants and SHcompact code.

`-no-expand`

  Do not expand MOVI, PT, PTA or PTB instructions.

`-expand-pt32`

  With -abi=64, expand PT, PTA and PTB instructions to 32 bits only.

`-h-tick-hex`

  Support H’00 style hex constants in addition to 0x00 style.

Next: SH64 Syntax, Up: SH64-Dependent [Contents][Index]