Next: File-I/O Remote Protocol Extension, Previous: Packet Acknowledgment, Up: Remote Protocol [Contents][Index]

### E.12 Examples

Example sequence of a target being re-started. Notice how the restart does not get any direct output:

    -> R00
    <- +
    target restarts
    -> ?
    <- +
    <- T001:1234123412341234
    -> +

Example sequence of a target being stepped by a single instruction:

    -> G1445…
    <- +
    -> s
    <- +
    time passes
    <- T001:1234123412341234
    -> +
    -> g
    <- +
    <- 1455…
    -> +