Next: File Transfer, Up: Remote Debugging [Contents][Index]

### 20.1 Connecting to a Remote Target

This section describes how to connect to a remote target, including the types of connections and their differences, how to set up executable and symbol files on the host and target, and the commands used for connecting to and disconnecting from the remote target.

#### 20.1.1 Types of Remote Connections

GDB supports two types of remote connections, `target remote` mode and `target extended-remote` mode. Note that many remote targets support only `target remote` mode. There are several major differences between the two types of connections, enumerated here:

Result of detach or program exit

  With target remote mode: When the debugged program exits or you detach from it, GDB disconnects from the target. When using `gdbserver`, `gdbserver` will exit.

  With target extended-remote mode: When the debugged program exits or you detach from it, GDB remains connected to the target, even though no program is running. You can rerun the program, attach to a running program, or use `monitor` commands specific to the target.

  When using `gdbserver` in this case, it does not exit unless it was invoked using the `--once` option. If the `--once` option was not used, you can ask `gdbserver` to exit using the `monitor exit` command (see Monitor Commands for gdbserver).

Specifying the program to debug

  For both connection types you use the `file` command to specify the program on the host system. If you are using `gdbserver` there are some differences in how to specify the location of the program on the target.

  With target remote mode: You must either specify the program to debug on the `gdbserver` command line or use the `--attach` option (see Attaching to a Running Program).

  With target extended-remote mode: You may specify the program to debug on the `gdbserver` command line, or you can load the program or attach to it using GDB commands after connecting to `gdbserver`.

  You can start `gdbserver` without supplying an initial command to run or process ID to attach. To do this, use the `--multi` command line option. Then you can connect using `target extended-remote` and start the program you want to debug (see below for details on using the `run` command in this scenario). Note that the conditions under which `gdbserver` terminates depend on how GDB connects to it (`target remote` or `target extended-remote`). The `--multi` option to `gdbserver` has no influence on that.

The `run` command

  With target remote mode: The `run` command is not supported. Once a connection has been established, you can use all the usual GDB commands to examine and change data. The remote program is already running, so you can use commands like `step` and `continue`.

  With target extended-remote mode: The `run` command is supported. The `run` command uses the value set by `set remote exec-file` (see set remote exec-file) to select the program to run. Command line arguments are supported, except for wildcard expansion and I/O redirection (see Arguments).

  If you specify the program to debug on the command line, then the `run` command is not required to start execution, and you can resume using commands like `step` and `continue` as with `target remote` mode.

Attaching

  With target remote mode: The GDB command `attach` is not supported. To attach to a running program using `gdbserver`, you must use the `--attach` option (see Running gdbserver).

  With target extended-remote mode: To attach to a running program, you may use the `attach` command after the connection has been established. If you are using `gdbserver`, you may also invoke `gdbserver` using the `--attach` option (see Running gdbserver).

#### 20.1.2 Host and Target Files

GDB, running on the host, needs access to symbol and debugging information for your program running on the target. This requires access to an unstripped copy of your program, and possibly any associated symbol files. Note that this section applies equally to both `target remote` mode and `target extended-remote` mode.

Some remote targets (see qXfer executable filename read, and see Host I/O Packets) allow GDB to access program files over the same connection used to communicate with GDB. With such a target, if the remote program is unstripped, the only command you need is `target remote` (or `target extended-remote`).

If the remote program is stripped, or the target does not support remote program file access, start up GDB using the name of the local unstripped copy of your program as the first argument, or use the `file` command. Use `set sysroot` to specify the location (on the host) of target libraries (unless your GDB was compiled with the correct sysroot using `--with-sysroot`). Alternatively, you may use `set solib-search-path` to specify how GDB locates target libraries.

The symbol file and target libraries must exactly match the executable and libraries on the target, with one exception: the files on the host system should not be stripped, even if the files on the target system are. Mismatched or missing files will lead to confusing results during debugging. On GNU/Linux targets, mismatched or missing files may also prevent `gdbserver` from debugging multi-threaded programs.

#### 20.1.3 Remote Connection Commands

GDB can communicate with the target over a serial line, or over an IP network using TCP or UDP. In each case, GDB uses the same protocol for debugging your program; only the medium carrying the debugging packets varies. The `target remote` and `target extended-remote` commands establish a connection to the target. Both commands accept the same arguments, which indicate the medium to use:

`target remote serial-device`
`target extended-remote serial-device`

  Use serial-device to communicate with the target. For example, to use a serial line connected to the device named `/dev/ttyb`:

      target remote /dev/ttyb

  If you’re using a serial line, you may want to give GDB the ‘`--baud`’ option, or use the `set serial baud` command (see set serial baud) before the `target` command.

`target remote `host:port``
`target remote `tcp:host:port``
`target extended-remote `host:port``
`target extended-remote `tcp:host:port``

  Debug using a TCP connection to port on host. The host may be either a host name or a numeric IP address; port must be a decimal number. The host could be the target machine itself, if it is directly connected to the net, or it might be a terminal server which in turn has a serial line to the target.

  For example, to connect to port 2828 on a terminal server named `manyfarms`:

      target remote manyfarms:2828

  If your remote target is actually running on the same machine as your debugger session (e.g. a simulator for your target running on the same host), you can omit the hostname. For example, to connect to port 1234 on your local machine:

      target remote :1234

  Note that the colon is still required here.

`target remote `udp:host:port``
`target extended-remote `udp:host:port``

  Debug using UDP packets to port on host. For example, to connect to UDP port 2828 on a terminal server named `manyfarms`:

      target remote udp:manyfarms:2828

  When using a UDP connection for remote debugging, you should keep in mind that the ‘U’ stands for “Unreliable”. UDP can silently drop packets on busy or unreliable networks, which will cause havoc with your debugging session.

`target remote | command`
`target extended-remote | command`

  Run command in the background and communicate with it using a pipe. The command is a shell command, to be parsed and expanded by the system’s command shell, `/bin/sh`; it should expect remote protocol packets on its standard input, and send replies on its standard output. You could use this to run a stand-alone simulator that speaks the remote debugging protocol, to make net connections using programs like `ssh`, or for other similar tricks.

  If command closes its standard output (perhaps by exiting), GDB will try to send it a `SIGTERM` signal. (If the program has already exited, this will have no effect.)

Whenever GDB is waiting for the remote program, if you type the interrupt character (often `Ctrl-c`), GDB attempts to stop the program. This may or may not succeed, depending in part on the hardware and the serial drivers the remote system uses. If you type the interrupt character once again, GDB displays this prompt:

    Interrupted while waiting for the program.
    Give up (and stop debugging it)?  (y or n)

In `target remote` mode, if you type `y`, GDB abandons the remote debugging session. (If you decide you want to try again later, you can use `target remote` again to connect once more.) If you type `n`, GDB goes back to waiting.

In `target extended-remote` mode, typing `n` will leave GDB connected to the target.

`detach`

  When you have finished debugging the remote program, you can use the `detach` command to release it from GDB control. Detaching from the target normally resumes its execution, but the results will depend on your particular remote stub. After the `detach` command in `target remote` mode, GDB is free to connect to another target. In `target extended-remote` mode, GDB is still connected to the target.

`disconnect`

  The `disconnect` command closes the connection to the target, and the target is generally not resumed. It will wait for GDB (this instance or another one) to connect and continue debugging. After the `disconnect` command, GDB is again free to connect to another target.

`monitor cmd`

  This command allows you to send arbitrary commands directly to the remote monitor. Since GDB doesn’t care about the commands it sends like this, this command is the way to extend GDB—you can add new commands that only the external monitor will understand and implement.

Next: File Transfer, Up: Remote Debugging [Contents][Index]