Next: MSP430-Chars, Up: MSP430 Syntax [Contents][Index]

#### 9.29.2.1 Macros

The macro syntax used on the MSP 430 is like that described in the MSP 430 Family Assembler Specification. Normal `as` macros should still work.

Additional built-in macros are:

`llo(exp)`

  Extracts least significant word from 32-bit expression ’exp’.

`lhi(exp)`

  Extracts most significant word from 32-bit expression ’exp’.

`hlo(exp)`

  Extracts 3rd word from 64-bit expression ’exp’.

`hhi(exp)`

  Extracts 4rd word from 64-bit expression ’exp’.

They normally being used as an immediate source operand.

        mov	#llo(1), r10	;	== mov	#1, r10
        mov	#lhi(1), r10	;	== mov	#0, r10