Next: Sbttl, Previous: Reloc, Up: Pseudo Ops [Contents][Index]

### 7.75 `.rept count`

Repeat the sequence of lines between the `.rept` directive and the next `.endr` directive count times.

For example, assembling

            .rept   3
            .long   0
            .endr

is equivalent to assembling

            .long   0
            .long   0
            .long   0

A count of zero is allowed, but nothing is generated. Negative counts are not allowed and if encountered will be treated as if they were zero.