Next: Loop Analysis and Representation, Previous: RTL, Up: Top [Contents][Index]

## 14 Control Flow Graph

A control flow graph (CFG) is a data structure built on top of the intermediate code representation (the RTL or `GIMPLE` instruction stream) abstracting the control flow behavior of a function that is being compiled. The CFG is a directed graph where the vertices represent basic blocks and edges represent possible transfer of control flow from one basic block to another. The data structures used to represent the control flow graph are defined in `basic-block.h`.

In GCC, the representation of control flow is maintained throughout the compilation process, from constructing the CFG early in `pass_build_cfg` to `pass_free_cfg` (see `passes.def`). The CFG takes various different modes and may undergo extensive manipulations, but the graph is always valid between its construction and its release. This way, transfer of information such as data flow, a measured profile, or the loop tree, can be propagated through the passes pipeline, and even from `GIMPLE` to `RTL`.

Often the CFG may be better viewed as integral part of instruction chain, than structure built on the top of it. Updating the compiler’s intermediate representation for instructions can not be easily done without proper maintenance of the CFG simultaneously.

Next: Loop Analysis and Representation, Previous: RTL, Up: Top [Contents][Index]