Next: AArch64 Mapping Symbols, Previous: AArch64 Directives, Up: AArch64-Dependent [Contents][Index]

#### 9.1.6 Opcodes

GAS implements all the standard AArch64 opcodes. It also implements several pseudo opcodes, including several synthetic load instructions.

`LDR =`

        ldr <register> , =<expression>

  The constant expression will be placed into the nearest literal pool (if it not already there) and a PC-relative LDR instruction will be generated.

For more information on the AArch64 instruction set and assembly language notation, see ‘`ARMv8 Instruction Set Overview`’ available at http://infocenter.arm.com.